*********************************************

Avago Technologies MegaRAID StorCLI Release 

*********************************************

Release Date: 06/23/17
========================

Supported Controllers
==================

MegaRAID SAS 9361-24i
MegaRAID SAS 9361-16i
Syncro 9361-8i
Syncro 9380-8e
MegaRAID SAS 9361-8i
MegaRAID SAS 9361-4i
MegaRAID SAS 9341-8i
MegaRAID SAS 9341-4i
MegaRAID SAS 9380-8e
MegaRAID SAS 9380-4i4e
MegaRAID SAS 9270-8i 
MegaRAID SAS 9271-4i 
MegaRAID SAS 9271-8i 
MegaRAID SAS 9271-8iCC 
Syncro CS 9271-8i
MegaRAID SAS 9286-8e 
MegaRAID SAS 9286CV-8e 
MegaRAID SAS 9286CV-8eCC
Syncro CS 9286-8e
MegaRAID SAS 9265-8i
MegaRAID SAS 9285-8e
MegaRAID SAS 9240-4i
MegaRAID SAS 9240-8i
MegaRAID SAS 9260-4i
MegaRAID SAS 9260CV-4i
MegaRAID SAS 9260-8i
MegaRAID SAS 9260CV-8i
MegaRAID SAS 9260DE-8i
MegaRAID SAS 9261-8i
MegaRAID SAS 9280-4i4e
MegaRAID SAS 9280-8e
MegaRAID SAS 9280DE-8e
MegaRAID SAS 9280-24i4e
MegaRAID SAS 9280-16i4e
MegaRAID SAS 9260-16i
MegaRAID SAS 9266-4i
MegaRAID SAS 9266-8i
MegaRAID SAS 9285CV-8e
MegaRAID SAS 9250-4i


Component:
=========
SAS MegaRAID StorCLI
Release Date: 06/23/17


Version Numbers:	StorCLI
===============		===========			
Current Version		1.23.02
Previous Versoin	1.21.06


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ01175605 -- storcli has an "=" (equal sign) as a reserved character and not allowed to be used as part of the ASO SafeStore
SCGCQ01280378 -- StorCLI /c0/dall show mirror command hits segmentation fault when no Drive Group on the controller
SCGCQ01282293 -- LibMods changes - Add OpenSSL v1.0.2i to StorCLI
SCGCQ01287099 -- storclif64.exe  show all says wrong Operating system name for Windows 2016.
SCGCQ01300711 -- Code changes for Big Endian servers for OS detection on the VD
SCGCQ01303002 -- Fixing resource leaks and invalid memory access
SCGCQ01288770 -- Storcli thorws wrong error message when tried import a saved config when VD is present


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.

Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.avagotech.com.

For the newer UEFI shells(shell version greater than 2.0), you should use the StorCli binary inside the UDK folder.
For Vmware binaries:
 _________________________________
|StorCli folder	|	OS Version|
|_______________|_________________|
|VMWare		|	VMWare 4.x|
|VMWare-MN	|	VMWare 5.x|
|VMWare-NDS	|	VMWare OP |
 ---------------------------------

=======================
Previous Releases
=======================


Component:
=========
SAS MegaRAID StorCLI
Release Date: 01/25/17


Version Numbers:	StorCLI
===============		===========			
Current Version		1.21.06
Previous Versoin	1.20.15


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ01167896 -- sparc version storcli tool can not execute storcli /cx show for intruder card
SCGCQ01201454 -- FRU info missing on oem and drives
SCGCQ01134166 -- Added new commands from StorCLI
SCGCQ01064480 -- MFI Frame alignment
SCGCQ01109142 -- RHEL 6.8: Storcli /c0 show all is not displaying OS driver version.
SCGCQ01144777 -- Adding CLI command to display/toggle  new controller property.
SCGCQ01144779 -- Libmod changes: Adding CLI command to display/toggle  new controller property
SCGCQ01079824 -- Storcli after Saving and Restoring configuration using file doesn't list EPD and JBOD in PDlist type
SCGCQ01134132 -- Add support for new version OpenSSL1.02g to support "DROWN" - CVE-2016-0800
SCGCQ01140805 -- Auto Learn Period displays only in days, extend it to hours , mins and sec
SCGCQ01144879 -- Add the force option sentence to consistent command for the output message
SCGCQ01145333 -- FW CLOSE is not send when FLASH DCMD fails with status MFI_STAT_LD_RECON_IN_PROGRESS
SCGCQ01167156 -- Defect SCGCQ01140805 needs to be fixed in EFI
SCGCQ01167240 -- Storcli fails to display  " ISE Capable " Field  for ISE drives
SCGCQ01154436 -- Application displays drives in unsorted manner wrt drive slot number
SCGCQ01185184 -- Removing the logically dead code from CLI.
SCGCQ01185666 -- Logically dead code, unused values and explicit NULL dereferences.
SCGCQ01185673 -- Removing the logically dead code from Libmods
SCGCQ01185690 -- Removed Missing return values in Libmods
SCGCQ01189619 -- Adding the code for Unchecked return values
SCGCQ01193194 -- storcli crashes while trying to load configuration
SCGCQ01195929 -- On performing a set personality to singlepdr0 the output under result column is show as singlepdr
SCGCQ01196785 -- Wrong error message is displayed on trying to create R0 vd on an pre configured drive as EPD.
SCGCQ01175605 -- storcli has an "=" (equal sign) as a reserved character and not allowed to be used as part of the ASO SafeStore
SCGCQ01202181 -- StorCLI help section needs to be updated
SCGCQ01210227 -- Storcli showing boot drive as EPDin JBOD personality
SCGCQ01210262 -- Storcli throws wrong error message and also shows Dual error messages in detailed status
SCGCQ01215128 -- add support check before set HDDThermalPollInterval and SSDThermalPollInterval in storcli
SCGCQ01215257 -- Updated the personality to switch between RAID and JBOD personality and allowing the behaviours of JBOD and None in JBOD personality.
SCGCQ01221627 -- Creating SecurityKey is not working when given with passphrasse or old-securityKey.


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.

Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.avagotech.com.

For the newer UEFI shells(shell version greater than 2.0), you should use the StorCli binary inside the UDK folder.
For Vmware binaries:
 _________________________________
|StorCli folder	|	OS Version|
|_______________|_________________|
|VMWare		|	VMWare 4.x|
|VMWare-MN	|	VMWare 5.x|
|VMWare-NDS	|	VMWare OP |
 ---------------------------------

=======================
Previous Releases
=======================






Component:
=========
SAS MegaRAID StorCLI
Release Date: 10/26/16


Version Numbers:	StorCLI
===============		===========			
Current Version		1.20.15
Previous Versoin	1.19.04


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ01017508 -- LibMods: Implement Process for testing SDS configurations / certifications
SCGCQ00988786 -- pinned cache of EPD generated listing as a VD under the description message of the preserved cache.
SCGCQ01023973 -- storcli command does not display the complete output
SCGCQ01023981 -- Changed all references of epdpassthru to JBOD
SCGCQ01023985 -- eSDS1.1:Not able to change the behavior mode through strocli
SCGCQ01024968 -- spell mistake(remaining time). in /c0/bbu show
SCGCQ01015016 -- Needs to be update the Description Status in Failure message of EPD delete
SCGCQ01015017 -- Segmentation fault(Core Dump) observed on executing command ./storcli /c0 show alilog.
SCGCQ01020010 -- Segmentation fault observed with multiple controllers with the command 'storcli /call show logfile=filename'
SCGCQ01015739 -- Add EPD, EPD-passthrough and single drive R0 behavior modes to ExpressSDS 1.1
SCGCQ01015758 -- OS_Utils: Multi-Path Support in EPD Config Options
SCGCQ01024964 -- HDD FW upgrades thru parallel loading of HDD microcode
SCGCQ01025826 -- Libmods changes for Multi-Path Support in EPD Config Options (ER SCGCQ01015758).
SCGCQ01023608 -- Custom CLI for OEM Solutions group
SCGCQ00865335 -- storcli /c0/pall show should have port no and is the port no valid which will help user to analyse the port#s.
SCGCQ00988786 -- SDS:  pinned cache of EPD generated listing as a VD under the description message of the preserved cache.
SCGCQ01021439 -- StorCLI shows inconsistent info for SSD Caching Enable/Disable in presence of max supported 64 VD's
SCGCQ01026081 -- Force is not working with parallel option in PD fw download
SCGCQ01026907 -- MR_6.12_StorCLI:Storcli vd hide giving error code even on success
SCGCQ01026945 -- Empty values are displayed after executing few commands in Storcli for value string in controller properties
SCGCQ01029534 -- Unable to set multipath parameter through storcli
SCGCQ01030139 -- "/c0 show events" shows the errMsg and ErrCd on command success.
SCGCQ01030430 -- StorCLI shows failure and success as output of PD FW flash command, when the flash has failed.
SCGCQ01030535 -- Mode 5 FW download is not working wth parallel
SCGCQ00994876 -- Info from CLI command for bbu  Mismatches with Firmware log
SCGCQ01029447 -- Storcli show personality displays "behavior" as "behaviour"
SCGCQ01031218 -- Application has Ambiguous behavior while PD FW flash and flash status check.
SCGCQ01033027 -- Printf seen in libmods in power-on-hours command
SCGCQ01033565 -- perccli .exe files are spelled wrong
SCGCQ01033794 -- MR6.12_StorCLI : Application shows two different status of a single operation on a PD connected in Multipath
SCGCQ01035493 -- Storcli output description asks for a system reboot when changing behavior from epd->r0
SCGCQ01036028 -- Segmentation fault seen while querying for preserved cache , while pinned cache is present.
SCGCQ01038696 -- IN JBOD mode under drive group topology RAID0 is shown
SCGCQ01039102 -- MR6.12:StorCLI displays wrong error message, when it tries to remove the Blocked Access from SVD's
SCGCQ01039484 -- Application shows FW flash status only for last drive when multiple drives are flashed simultaneously
SCGCQ01039534 -- Storcli does not give context specific output for the storcli help commands
SCGCQ01039536 -- Mri mode is taking any value and not reflecting
SCGCQ01039554 -- Calculate the Leap year information for show alilog command
SCGCQ01039745 -- MR6.12_Arm_Storcli.efi: Help does not work for storcli.efi /c0 h
SCGCQ01039756 -- MR6.12_Arm_Storcli.efi:No error message shown when deleting securitykey fails
SCGCQ01039757 -- MR6.12_Arm_storcli.efi:Error Message Wrong on start learn cycle failure scenario
SCGCQ01039758 -- Application to show precise failure message for VD add when background operations in progress.
SCGCQ01041178 -- Storcli reports wrong 'model no' for the PD which is in the UBad state- storcli /c0 show page
SCGCQ01043063 -- MR6.12_Storcli_arm:Error message not proper when foreign config delete attempted in safe mode
SCGCQ01044939 -- Factory settings changes for Transport as per new MFC_DEFAULTS in API.
SCGCQ01047957 -- Global Hot Spares shows as TR in storcli DG query when TR is activated on DG
SCGCQ01049064 -- StorCLI show phyerrorcounters command does not display any PHY Error Counter Values
SCGCQ00929757 -- Request to add" Secure Erase" support to JBOD/System drives
SCGCQ01026250 -- Support ARM processors  on EFI platform
SCGCQ01040304 -- Display PR progress in storcli
SCGCQ01047223 -- OS_Utilsl: Drive FW update. Mode E and F
SCGCQ01047229 -- added a entity JBOD for the various operation on these JBOD?s.
SCGCQ01038669 -- StorCLI /c0 show phyerrorcounters Success without table  in Linux/FreeBSD/Solaris 32-bit version
SCGCQ01050695 -- Changed the command status as "success"
SCGCQ01050766 -- eSDS1.1: Add EPD allowed in JBOD mode
SCGCQ01052306 -- MR6.12_Arm_Storcli:/c0/dall set command gets executed succesfully
SCGCQ01052322 -- MR_6.12_Arm_storcli.efi: Controller restart command success in the EFI and the system hangs
SCGCQ01052841 -- storcli /c0 dall show is hanging or throwing exception
SCGCQ01052876 -- storcli /c0 show displays JBOD list when the behavior is in EPD
SCGCQ01052895 -- When activatenow is specified with no delay, Mode F does not get fired after Mode E.
SCGCQ01053068 -- Mode E and F firmware download: In case Mode E/F fails, we need to disable offline command and then exit.
SCGCQ01053241 -- 6.12_StorCLI : Application shows wrong message when boot drive is cleared on all PDs.
SCGCQ01053608 -- MR6.12_Storcli: Storcli Copyright shows 2015 instead of 2016
SCGCQ01057994 -- VD erase with pattern is deleting the volume
SCGCQ01058116 -- Description  should be more accurate for strocli /c0/vall show all command
SCGCQ01058178 -- JBOD is specified even though the entity here is EPD. The table should display EPD and not JBOD.
SCGCQ01058298 -- MR_6.12_ARM_Storcli.efi:storclio.efi /c0 set pcilinkspeed=3 success and set as 3%
SCGCQ01058300 -- MR_6.12_Arm_Storclio.efi:Set MFG data shows success if input some invalid file.
SCGCQ01058525 -- controller show memscrubpatterns status show succes and descriptions says failed.
SCGCQ01059088 -- whiel Querying EPD info JBOD is getting displayed
SCGCQ01059105 -- complete error message is not shown when trying to update the security key "rekeyLock "
SCGCQ01050234 -- New option for hide/unhide option on a DiskGroup.
SCGCQ01061120 -- MR 6.11 Sparc:Segmentation fault(Core Dump) observed on executing command ./storcli /c0 show dequeuelog file=filename.txt
SCGCQ00804672 -- Non-array delete for objects: destructors will not be called for objects in the array leading to unexpected behaviour.
SCGCQ01028468 -- StorCLI crashes, while enabling/disabling SSDCaching on max supported SVD's
SCGCQ01053241 -- 6.12_StorCLI : Application shows wrong message when boot drive is cleared on all PDs.
SCGCQ01062314 -- Jbod status is shown under EPD column while displaying the status message
SCGCQ01063305 -- MR_6.12_storcli: Segmentation fault found while starting recon operation with more than 100 drives
SCGCQ01063899 -- MR6.12_Storcli: While dumping the logs, on giving wrong destination storcli doesnt throw any error
SCGCQ01064028 -- CLI - Shows (cx/epdx show) Port information as "Port 0-3 x4" / "Port 4-7 x4" against an EPD instead of "Port 0-3"/"Port 4-7"
SCGCQ01064035 -- CLI - Shows BBMT information against EPDs when query "/Cx/Vall show BBMT"
SCGCQ01064084 -- storcli throws wrong error message while creating VD
SCGCQ01064101 -- JBOD information is displayed in EPD mode
SCGCQ01064736 -- MR6.12_StorCLI : With bad drive in config, application shows wrong message when trying to add VD.
SCGCQ01064750 -- eSDS_1.1_Alpha : Storcli doesnot display driver version for linux 32 bit
SCGCQ01064773 -- Need to remove space before the comma in the sentence "Flash image is not supported , Try force."
SCGCQ01066153 -- UDK version of Storcli.efi (1.18.05) updates non existent storage adapters and causes the system to hang
SCGCQ01066204 -- MR 6.12 Alpha CLI Solaris:PD firmware flash with parallel option returns error code 18
SCGCQ01067274 -- Strocli displays Nytrocache, caches flushed successfully for MR controllers
SCGCQ01068420 -- StorCLI enclosure show different information for  a PD connected in multipath
SCGCQ01070120 -- Improper handling of MFC_DEFAULTS in VD creation
SCGCQ00892905 -- Retrieving phyerrorcounters of the enclosure failed in Linux 32
SCGCQ01061212 -- Extra characters are displayed with /c0/eall show all
SCGCQ01065620 -- storcli: on trying to flash the wrong drive FW on a pd, storcli throws inappropriate error message
SCGCQ01073669 -- MR6.12_Storcli: Storcli throws wrong error message while creating VD using online drives
SCGCQ01074482 -- eSDS_1.1_HSW_Beta: Storcli set CC is failing with status failure, but it is setting the CC
SCGCQ01074514 -- MR 6.12 Beta Storclio: Installation of storclio fails with syntax error in Solaris sparc 11.3.
SCGCQ01075118 -- ./storcli /c0/fall show displays raid level as raid 0 for any raid level in foreign state.
SCGCQ01078549 -- MR_6.12_Arm_StorcliO.EFI:Junk Characters are displayed while attempting to create more than 64 VD's in a drive group
SCGCQ01078997 -- Multi Init param help syntax missing
SCGCQ01079423 -- MR6.12_StorCLI : Segmentation fault seen when 64VDs with IOs is deleted and enclosure is removed.
SCGCQ01079667 -- Storcli set jbod as boot drive and removing jbod as boot drive is displaying two different messages.
SCGCQ01080489 -- On setting lowlatency to OFF the multipath which was set to ON earlier is also set to OFF.
SCGCQ01080493 -- Storcli switching personality behavior from JBOD and EPD to none is not clearing JBOD and EPD config.
SCGCQ01081082 -- Mr_6.12_Arm_StorCLI.EFI:Synchronous Exception on giving more than 200 characters in storcli command
SCGCQ01082500 -- MR 6.12 storclio: sasaddress mismatch after setting sasaddress from storclio.
SCGCQ01085706 -- MR612_StorCLI : Application does not allow to flash SATA SSD FW.
SCGCQ01091011 -- MR612_StorCLI : Application displays extra prints, incorrect messages while flashing PD FW on SAS/SATA
SCGCQ01054880 -- MR 6.12 Alpha Solaris 11.3 lmrc:./storcli /c0/ex show phyerrorcounters" returns failed to get phyerror info in solaris11 x86
SCGCQ01077590 -- MR 6.12 Beta CLI:/storcli /cx/ex show phyerrorcounters fails to fetch phyerror info of enclosure in Solaris Sparc 11.3
SCGCQ01091178 -- CLI output is not consistent on clearing the config
SCGCQ01107558 -- MR 6.12 Storcli Sparc:./storcli /cx/ex/sx show smart displays null value under smart data info.
SCGCQ01125454 -- Storcli reports empty Firmware Release Number on a SAS drive
SCGCQ01132613 -- Storcli not handling the return status during controller firmware flash
SCGCQ01133117 -- MR_6.13: Storcli App throws an error message disable PI command fails, but in FW/MSM seen Data protection is disabled.
SCGCQ01137070 -- Storcli is allowing write back vd creations when in HBA personality
SCGCQ01127378 -- Storcli menu still displays SDS reference and multiple modes for personality switch
SCGCQ01131493 -- Help file is not available for storcli /c0 add jbod h
SCGCQ01146775 -- Added the code to display the JBOD personality and switch between the JBOD and RAID personalities
SCGCQ01146776 -- Added the code to display the JBOD personality and switch between the JBOD and RAID personalities




Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.

Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.avagotech.com.

For the newer UEFI shells(shell version greater than 2.0), you should use the StorCli binary inside the UDK folder.
For Vmware binaries:
 _________________________________
|StorCli folder	|	OS Version|
|_______________|_________________|
|VMWare		|	VMWare 4.x|
|VMWare-MN	|	VMWare 5.x|
|VMWare-NDS	|	VMWare OP |
 ---------------------------------




Component:
=========





SAS MegaRAID StorCLI
Release Date: 03/21/16


Version Numbers:	StorCLI
===============		===========			
Current Version		1.19.04
Previous Versoin	1.18.05


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00861227 - (Closed) - storcli gives a success message even when the logfile's destination doesnt have any storage space to save the file. 
SCGCQ00940074 - (Closed) - Create 64 VDs in MR. Degrade the config. Bring the config to iMR and issue /c0/fall show /c0/fall show succeeds Issue /c0/fall show all. It fails. 
SCGCQ00950438 - (Closed) - Storcli displays enclosure many fields information as "Unsupported"
SCGCQ00981663 - (Closed) - Storcli to fail the transport DG when user requests only shared but a dedicated HSP is present 
SCGCQ00995140 - (Closed) - Wrong message displayed while R5 creation
SCGCQ00995154 - (Closed) - VD Loss observed after starting erase operation on R0 VD in simple and normal mode. 
SCGCQ00997401 - (Closed) - Extra print of "File Write ERROR !!! " comes when retentiontest command is executed in storclio.efi 
SCGCQ00999258 - (Closed) - Storcli gives wrong failure message if tried to create R1 with 3 drives
SCGCQ01000358 - (Closed) - VD Policy can't be retained after false FW flash
SCGCQ01003956 - (Resolved) - warning: file /opt/MegaRAID/storcli/storcli: remove failed: No such file or directory; while uninstalling StorCLI 1.18.08
SCGCQ01014101 - (Closed) - Segmentation fault(Core Dump) observed on executing command ./storcli /c0 show alilog. 
SCGCQ00993464 - (Closed) - storcli fails to set JBOD=off when there are no JBOD's too
SCGCQ00993466 - (Closed) - Force Flash is not working with resetnow option
SCGCQ01003415 - (Closed) - Application shows inappropriate message when trying to configure R0 with online PDs. 
SCGCQ00890604 - (Closed) - Connector name is not in sorted state when queried from storcli . Ports displays in descending order 
SCGCQ00973474 - (Closed) - MR6.10.5 Storcli misspelling of 'Cotroller' when flushing controller 
SCGCQ01019547 - (Closed) - Segmentation fault observed with multiple controllers with the command 'storcli /call show logfile=filename' 
SCGCQ00952422 - (Closed) - MR 6.11 CLI: Installation of storclio fails on Solaris SPARC 11.3
SCGCQ00890597 - (Closed) - Connector name for first 8 PHY for enclosure is not displayed as it has to be
SCGCQ00920058 - (Implemented) - Standard Support for SPARC Solaris
SCGCQ00953464 - (Active) - Connector name for first 8 PHY for enclosure is not displayed as it has to be
SCGCQ00998120 - (Port_Complete) - Checking-in CLI changes for defect SCGCQ00997174
SCGCQ01004630 - (Port_Complete) - "Storcli show" command is failing with Intruder 
SCGCQ01004610 - (Port_Complete) - Modified the failure message as per user-requested message as "This command only applies to Nytro Megaraid controllers. All others will display a failure status."



Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.

Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.avagotech.com.

For the newer UEFI shells(shell version greater than 2.0), you should use the StorCli binary inside the UDK folder.
For Vmware binaries:
 _________________________________
|StorCli folder	|	OS Version|
|_______________|_________________|
|VMWare		|	VMWare 4.x|
|VMWare-MN	|	VMWare 5.x|
|VMWare-NDS	|	VMWare OP |
 ---------------------------------





Component:
=========
SAS MegaRAID StorCLI
Release Date: 12/30/15


Version Numbers:	StorCLI
===============		===========			
Current Version		1.18.05
Previous Versoin	1.17.08


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00894452 - (Closed) - Storcli displays wrong message while deleting a CCVD
SCGCQ00894601 - (Closed) - StorCLI : output string needs to be change for largeIO support command
SCGCQ00898456 - (Closed) - MR: on converting the UG drives to UG again, storlci throws inappropriate message
SCGCQ00898881 - (Closed) - MR_Intruder_6_9_Storcli: Segmentation fault is obeserved while quering for enclosure details.
SCGCQ00914349 - (Closed) - MR 6.10 : Unit for Capacitance value is not shown storcli /c0/cv show all.
SCGCQ00916693 - (Closed) - MR_6.10_storcli: In perfmode 'numOrderIOs' can't be set beyond 25
SCGCQ00919988 - (Closed) - Storclif thowing an error while issuing the command "Set factory file=mfc.ini"
SCGCQ00940074 - (Closed) - Create 64 VDs in MR. Degrade the config. Bring the config to iMR and issue /c0/fall show /c0/fall show succeeds Issue /c0/fall show all. It fails.
SCGCQ00893958 - (Closed) - MR_Intruder: Incomplete help file provided for the command storcli /cx set autopdcache=<off|[on|sscr0]|r0|wbr0> [immediate]
SCGCQ00914834 - (Closed) - Updating storcli as per the API changes for LargeIOSupport
SCGCQ00915523 - (Closed) - Resoure leaks while performing the volume deletion
SCGCQ00917235 - (Closed) - Fix resource creation NULL check in the code
SCGCQ00904416 - (Closed) - setting jbodwritecache to enabled or disabled appears to work but it can only be set to "Disks Default"
SCGCQ00904724 - (Closed) - on giving the same vd number multiple time while deleting will lead to segmentation fault
SCGCQ00927102 - (Closed) - MR_6.10_storcli: Storcli displays wrong failure message while setting cbsize
SCGCQ00890604 - (Closed) - Connector name is not in sorted state when queried from storcli . Ports displays in descending order
SCGCQ00904342 - (Closed) - CC delays get unset when CC mode is changed
SCGCQ00904379 - (Closed) - Montask at diagRetentionCmdBlockDone+1c0 while running retentiontest through storclio
SCGCQ00904662 - (Closed) - Updating the BBU-properties(BBU learn mode)
SCGCQ00907610 - (Closed) - StorCLI_Intruder: The assignvds field for add Cachecade fails if there are VD holes instead of continuing with rest of the VD
SCGCQ00917277 - (Closed) - MR 6.10 Alpha Storcli: Spelling mistake in description "Adapter 'configuaration' Failed" while loading configuration.
SCGCQ00904794 - (Closed) - Updating the default the write policy for VD creation
SCGCQ00890597 - (Closed) - Connector name for first 8 PHY for enclosure is not displayed as it has 
SCGCQ00867500 - (Closed) - Request to add retentiontest comman to storclio
SCGCQ00920046 - (Implemented) - Added the support to set and clear the transport on a DG either by including/excluding hotspares.
SCGCQ00933318 - (Implemented) - Added the support to swtich the large queue depth ctrl property in storcli
SCGCQ00894103 - (Closed) - StorCLI : Add support to enable/Disable of Large IO Support - 1 M
SCGCQ00894644 - (Port_Complete) - StorCLI : Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00912699 - (Port_Complete) - Stop_resume_pasue Help description needs to corrected
SCGCQ00912696 - (Port_Complete) - Spelling mistakes in verbose help for /cx ,/sx,/ex
SCGCQ00912559 - (Port_Complete) - Description is none for Invalid stripe size while creating VD with storcli
SCGCQ00915468 - (Port_Complete) - Updating storcli as per the API changes for LargeIOSupport
SCGCQ00895075 - (Active) - Estimated time left for Init op is blank in storcli for Falcon cards
SCGCQ00907178 - (Active) - setting jbodwritecache to enabled or disabled appears to work but it can only be set to "Disks Default"
SCGCQ00912704 - (Port_Complete) - Need to Correct spelling mistake in help file of show events
SCGCQ00912762 - (Port_Complete) - Fix for help contents for ./storcli64 /c0/fall import command
SCGCQ00924705 - (Port_Complete) - CLI downgrades FW without notifying user of earlier version or requiring noverchk command
SCGCQ00904668 - (Port_Complete) - Updating the BBU-properties(BBU learn mode)
SCGCQ00912701 - (Port_Complete) - Detailed Help of set command have few spelling mistakes (to corrected "specfied ").
SCGCQ00897816 - (Port_Complete) - MR_Intruder: Incomplete help file provided for the command storcli /cx set autopdcache=<off|[on|sscr0]|r0|wbr0> [immediate]
SCGCQ00928760 - (Port_Complete) - SDS:Delete preservedcache option is not listing in main help of "/c0/vx delete h"
SCGCQ00912727 - (Port_Complete) - observed spelling mistake in help file of the command "storcli /c0 show bootdrive h"
SCGCQ00912714 - (Port_Complete) - Detailed Help of show command have few spelling mistakes (to corrected "possiblities").
SCGCQ00897785 - (Port_Complete) - Storcli displays wrong message while deleting a CCVD
SCGCQ00912658 - (Port_Complete) - Inconsistent behavior observed in StorCLI, on Show rebuild progress command.
SCGCQ00912723 - (Port_Complete) - observed spelling mistake in help file of the command "storcli /c0 show pdfaileventoptions
SCGCQ00912719 - (Port_Complete) - Detailed Help of add command have few spelling mistakes (to be corrected for "convension","Speciifes "ceration "
SCGCQ00912693 - (Port_Complete) -  Spelling Mistake to be corrected in detailed help file vx_dx_fall_bbu_cv details.
SCGCQ00904796 - (Port_Complete) - Updating the default the write policy for VD creation
SCGCQ00900085 - (Port_Complete) - Method field is empty for most of the "storcli /c0 show events" command & some of the output are misaligned
SCGCQ00904360 - (Active) - CC delays get unset when CC mode is changed
SCGCQ00912709 - (Port_Complete) - Need to Correct spelling mistake in output of PHY linkspeed
SCGCQ00912657 - (Port_Complete) - Foreign VD count of spanned drive group is inconsistent i:e it is considering twice for the spanned drive groups
SCGCQ00900086 - (Port_Complete) - Method field is empty for most of the "storcli /c0 show events" command & some of the output are misaligned
SCGCQ00912801 - (Active) - CISCO_EPMR8: Abbreviations missing in output command of "/c2/e45/s1 show phyerrorcounters"
SCGCQ00895074 - (Active) - Estimated time left for Init op is blank in storcli for Falcon c




Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.




Component:
=========
SAS MegaRAID StorCLI
Release Date: 10/05/15


Version Numbers:	StorCLI
===============		===========			
Current Version		1.17.08
Previous Versoin	1.16.06


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00845688 - (Closed) - MR_6.8_storcli: Fails to get phyerrorcounters of the expander phys for the enclosures which are in daisy chain
SCGCQ00853174 - (Closed) - Storcli writes "no CC errors were logged " instead of "no pd events" in a file, when fire a command pdfailevents.
SCGCQ00857748 - (Closed) - On executing storcli cmd to dump alilog, it posts an error message and also doesnt list all the information
SCGCQ00857760 - (Closed) - Alignment of logs in the log file for the controller info is not proper
SCGCQ00863767 - (Closed) - Fixed all the resource leaks, Null pointer deferences and error handling issues.
SCGCQ00865020 - (Closed) - The Design Info field is partially populated for CV in StorCLI Ver 1.17.01 as compared to the previous releases.
SCGCQ00874043 - (Closed) - StorCLI returns confusing message when flashing incompatible FW image(16MB)
SCGCQ00880288 - (Closed) - storcli command "/c0 show alilog" takes more than 2 mins.
SCGCQ00880959 - (Closed) - Coverity defect fixes in Storcli 6.9
SCGCQ00884900 - (Closed) - Coverity defects in 6.9 Storlci
SCGCQ00894452 - (Closed) - Storcli displays wrong message while deleting a CCVD
SCGCQ00894601 - (Closed) - StorCLI : output string needs to be change for largeIO support command
SCGCQ00845602 - (Closed) - Alpha 6.8: Storcli command ./storcli /cx/fall show not displaying proper error message for non importable VD.
SCGCQ00859728 - (Closed) - Need to change the message if identified an OS or file system on VD
SCGCQ00867587 - (Closed) - Check for OS on any Jbod while disabling JBOD on the controller
SCGCQ00914834 - (Closed) - Updating storcli as per the API changes for LargeIOSupport
SCGCQ00860801 - (Closed) - Coverity defects for 6.9
SCGCQ00863669 - (Closed) - Coverity fixes in MR6.9
SCGCQ00865464 - (Closed) - Incorrect error message displays BBU instead of CV
SCGCQ00874608 - (Resolved) - misspelled word in storcli message
SCGCQ00893958 - (Resolved) - MR_Intruder: Incomplete help file provided for the command storcli /cx set autopdcache=<off|[on|sscr0]|r0|wbr0> [immediate]
SCGCQ00865804 - (Closed) - PERCCLI shows storccli during help command
SCGCQ00865971 - (Closed) - StorCLI saves a degraded config but does not restore it.
SCGCQ00873650 - (Closed) - Dereferencing the null pointer
SCGCQ00855390 - (Closed) - Adding NULL Check to avoid referencing a NULL
SCGCQ00860822 - (Closed) - If connector index is 0xFF display connector name as "Internal"
SCGCQ00864791 - (Closed) - Coverity defects(Adding NULL Checks and Error messages in failure cases)
SCGCQ00853185 - (Closed) - Storcli fails to dump lastoneday pdfailevents in a file.
SCGCQ00855389 - (Closed) - Remove unused variables in flash Cp.
SCGCQ00877894 - (Closed) - Disable SSD caching fails from Storcli in OEL 7.
SCGCQ00873620 - (Closed) - StorCLI does not find enclosures in multipath environme
SCGCQ00851795 - (Implemented) - Implemented commands to save/restore the configuration on the controller.
SCGCQ00867424 - (Implemented) - Incorrect message displayed when performing Auto configuration raid 0 with SSD drives.
SCGCQ00828030 - (Implemented) - Add support to detect that an OS is installed on a JBOD and to block it from being changed to Unconfigured Good
SCGCQ00894103 - (Closed) - StorCLI : Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00854620 - (Implemented) - Provide a more descriptive port enumeration
SCGCQ00833594 - (Closed) - added new command /c0 show swalilog equivalent to adpalilog
SCGCQ00850619 - (Closed) - Added support for flashing the FW on intruder and new Dev-ID's of Invader are added f
SCGCQ00853554 - (Port_Complete) - OEM requesting to do a WRITE VERIFY prior to flushing cache.
SCGCQ00864789 - (Port_Complete) - Spelling mistake in storcli output command pdfaileventoption



Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.




SAS MegaRAID StorCLI
Release Date: 07/13/15


Version Numbers:	StorCLI
===============		===========			
Current Version		1.16.06
Previous Versoin	1.15.05


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00355536 - (Closed) - MegaCli and StorCli can not manage both Liberator (and prior) and TB controllers in the same system under FreeBSD with the mf
SCGCQ00357948 - (Closed) - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
SCGCQ00359629 - (Closed) - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
SCGCQ00359998 - (Closed) - Code clean up in libmods and sysefi files are added
SCGCQ00360814 - (Closed) - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
SCGCQ00362216 - (Closed) - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
SCGCQ00362717 - (Closed) - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
SCGCQ00363455 - (Closed) - The legend for the PD List table exceeds 80 char limit.
SCGCQ00363522 - (Closed) - storcli query for displaying controller properties is showing status , as failure.
SCGCQ00364248 - (Closed) - StorCLI failed to delete a VD that is just created under Windows 2008
SCGCQ00364622 - (Closed) - Reports wrong diskgroup size while querying controller level properties
SCGCQ00364735 - (Closed) - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
SCGCQ00371445 - (Closed) - Vmware CLI fails to set the phy linkspeed
SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00381100 - (Closed) - MR: not able to create PRL11 using 96 drives.
SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00475583 - (Closed) - Raptor_Galaxy_Tencent:Tencent Storcli detecting the card.
SCGCQ00479843 - (Closed) - Storcli internal errors should return with 1001, but its coming as -1
SCGCQ00481474 - (Closed) - Some Numeric values in CLI o/p comes in Hex format
SCGCQ00484560 - (Closed) - Try to create a Exclusive VD, but after creation it still shows as Shared VD.
SCGCQ00505771 - (Closed) - Wrong size of CacheCade VD is getting displayed after making one PD offline
SCGCQ00518543 - (Closed) - PCLI Sparc(1.07.02):" Cli show all" command fails with error msg "Error! App exec failed in FW PCLIError! Internal".
SCGCQ00568073 - (Closed) - Storclio_1.09.00:Fails to set SubOEMID on Solaris OS .
SCGCQ00574835 - (Closed) - MR_Inv_6.3_PPC:Storcli- Retreiving LDBBM info through storcli is failing on SLES11 SP2 PPC64
SCGCQ00579658 - (Closed) - PPC64 :: MR Liberator :: All commands of StorCli is failing with segmentation fault after creating a GlobalHotSpare
SCGCQ00644123 - (Closed) - "/cx/ex show phyerrorcounters" gives core dump on freeBSD 32 and 64 bit.
SCGCQ00653742 - (Closed) - Storlib header file checkin and make compatible changes in CLI code.
SCGCQ00690355 - (Closed) - Storcli shows two controllers in the system though you have only one cotntroller in the system.
SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
SCGCQ00725192 - (Closed) - H330: Firmware Crash is hit while creating the Raid1 vd without drives selected
SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
SCGCQ00784808 - (Closed) - "cpybck" help is not coming in Legends
SCGCQ00792202 - (Closed) - Readability : Output string need to be updated for supportForceTo512e in show all command
SCGCQ00792232 - (Closed) - MFCdefaults : DisableHII option needs to be include in getShowDefaults()
SCGCQ00793374 - (Closed) - Comparing an array to null is not useful: "rawSmartData != NULL"
SCGCQ00794394 - (Closed) - MR_6.7_STROCLI: Command "./storcli64 /c0/ex/sx reset phyerrorcounters" fails in RHEL6.6 PPC64
SCGCQ00802031 - (Closed) - Deallocation of the same memory more than 
SCGCQ00804554 - (Closed) - emory not freed which can cause leak
SCGCQ00804588 - (Closed) - Memory leak happening in failure case since not freeing before returning error code.
SCGCQ00818653 - (Closed) - Copyright value still shows 2014
SCGCQ00827049 - (Closed) - Storcli cannot create R10 in iMR with 6 or 8 drives per span.
SCGCQ00827299 - (Closed) - Storcli crashes instead of showing error message on enabling caching on Source VDs and C
SCGCQ00833223 - (Closed) - Not displaying the timePeriod for event MR_EVT_PD_DEGRADED_MEDIA_POOR_PERFORMANCE
SCGCQ00833224 - (Closed) - setting vfmap with PF/wrong VF is throwing error
SCGCQ00839797 - (Closed) - Segmentation Fault observed, when trying to create R1 CCVD using 3/5 drives
SCGCQ00840948 - (Closed) - Storcli throws syntax error,when setting errorThreshold.
SCGCQ00853174 - (Closed) - Storcli writes "no CC errors were logged " instead of "no pd events" in a file, when fire a command pdfailevents.
SCGCQ00360040 - (Closed) - Storcli is returning error with show
SCGCQ00362070 - (Closed) - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
SCGCQ00362421 - (Closed) - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit)
SCGCQ00364097 - (Closed) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00365632 - (Closed) - PCI Info for FreeBSD needs to be indicated as "N/A"
SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00378135 - (Closed) - portings of AdpRestart command
SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00424978 - (Closed) - MR6.1: Hamlin: Is VD Emulated=Yes when emulationType=1
SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00490620 - (Closed) - Unable to insert a drive after setting a drive as 'Missing' .
SCGCQ00503981 - (Closed) - Command "./Storcli /call/eall/sx set offline" fails with ERRcode1001 and ERRmsg drive not found.
SCGCQ00504585 - (Closed) - Some sparc structures missing for storcli.
SCGCQ00567761 - (Closed) - MR Liberator : PPC SERVERGY Server : MonTask: line 541 in file ../../raid/raidpci.c
SCGCQ00644545 - (Closed) - storecli reports wrong size on 3000MB VD
SCGCQ00649324 - (Closed) - MR6.4_StorCLI_240VD: StorCLI crashes on issuing /c1 set cc=conc delay=10 starttime=2014/12/12 12 excludevd=0
SCGCQ00649962 - (Closed) - Cannot create a VD smaller than 800MB with 4K drives
SCGCQ00653672 - (Closed) - MR6.4: Storcli show command does not display all the controllers plugged into the server
SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
SCGCQ00785918 - (Closed) - Reviewing the Code AdataMfi, RmDataMf and VdDataMf files.
SCGCQ00792200 - (Closed) - supportCPLDUpdate support bit needs to be updated in contoller detailed information
SCGCQ00793761 - (Closed) - The HDD firmware revision is shown blank for few drives connected.
SCGCQ00794393 - (Closed) - MR_6.7_STROCLI: "./storcli64 /c0/ex show phyerrorcounters" gives segmentation fault in RHEL6.6 PPC64
SCGCQ00795335 - (Closed) - Explicit null dereferenced in rmdatamf.cpp causing wrong result
SCGCQ00796206 - (Closed) - fisResBuffer memory allocation is not considering the failure case
SCGCQ00803420 - (Closed) - Storcli displays wrong native driver version on ESXi5.5 when quered .
SCGCQ00804745 - (Closed) - Resource leak - Leak of memory or pointers to system resources
SCGCQ00805547 - (Closed) - MR_6.7_ Storcli: "Storcli /cx/eall/sall show " gives no enclosure found if two enclosures are connected in multipath scenario
SCGCQ00806966 - (Resolved) - IDA show incorrect RAID controller type information
SCGCQ00814939 - (Closed) - MR_6.7: Storcli Command "./storcli /c0/v2 set accesspolicy=RmvBlkd " fails for a blocked source VD.
SCGCQ00819880 - (Closed) - Gas Gauge Update + StorCLI ResetNow Op
SCGCQ00837197 - (Closed) - MR_6.8_Storcli: Cachevault flash size shows differently for different commands in storcli under RHEL6.6 PPC64
SCGCQ00837339 - (Closed) - "/c0/cv show all" shows "CacheVault Flash Size" as 0KB for TB.
SCGCQ00837342 - (Closed) - New PD_Degraded media events are not logging correctly in PPC
SCGCQ00840408 - (Closed) - Storcli gives wrong message for '/c1 /eall show phyerrorcounters' on IMR controller with no enclosures
SCGCQ00357263 - (Closed) - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
SCGCQ00366000 - (Closed) - Storcli displays incomplete serial number for some SSDs
SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite IBM Flatwood controller having power saving option completely disabled.
SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
SCGCQ00475562 - (Resolved) Storcli - DFF firmware download fails with config ID mismatch on ESXi5.1
SCGCQ00475815 - (Closed) - debug prints are present when issuing /co/eall show
SCGCQ00499067 - (Closed) - Storcli reports VD Type as "Rec1" during reconstruction on SPARC.
SCGCQ00518579 - (Closed) - Unable to make R10 through Ctrl R using 4k drives
SCGCQ00529763 - (Closed) - Some characters missing while querying for VD properties with having 64 VD's on a controller.
SCGCQ00572800 - (Closed) - MR_Inv_6.3_PPC:Storcli-WWN is showing blank for SAS PDs on SLES11 SP2 PPC64
SCGCQ00581416 - (Closed) - PPC64 :: MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
SCGCQ00601775 - (Closed) - MR : on querying PR status, storcli hits segmentation fault.
SCGCQ00609942 - (Closed) - storelib header file changes porting
SCGCQ00645195 - (Closed) - Storcli : unable to set patrol read delay
SCGCQ00674023 - (Closed) - MR_6.4_StorCli_EFI: Storcli.efi crashes for iMR card.
SCGCQ00674969 - (Closed) - Storcli doesn't show SN of Samsung SSD 200/400/800 in SWRAID version 1.32
SCGCQ00695070 - (Closed) - storcli /c0 show all is not displaying "support vd hide" and "support HOQrebuild" feilds and legends are not displayed for HD
SCGCQ00729691 - (Closed) - MR6.5alpha:Segmentation fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
SCGCQ00792264 - (Closed) - Missing the Display of the property temperatureCtrl.
SCGCQ00794760 - (Closed) - When Supercap SOH is reported bad, CLI still see the Supercap status as "Optimal"
SCGCQ00799426 - (Closed) - Command /cx/ex show phyerrorcounters gives bus error in Orcale Enterprise Linux
SCGCQ00804650 - (Closed) - Varailble need to be freed before returning in all failure case
SCGCQ00809736 - (Closed) - FW hangs during SVD and CCVD migration based on DDR Size
SCGCQ00830544 - (Closed) - Adpalilog is failing with storcli
SCGCQ00838307 - (Closed) - Maintainer name being populated while querying for storcli version from OS
SCGCQ00840372 - (Closed) - Read policy should be 'NORA' for IMR controller instead of 'none'
SCGCQ00842237 - (Closed) - storcli exits with legacy syntax for pdfwdownload
SCGCQ00357913 - (Closed) - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
SCGCQ00360745 - (Closed) - StorCLI does not provide command to set HSM or HCOE SCGCQ00358662
SCGCQ00364332 - (Closed) - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00365950 - (Closed) - StorCLI cannot displays information for controller in Safe mode
SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00384644 - (Closed) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00465956 - (Closed) - No of blocks displayed for a VD remains same for all VD sizes.
SCGCQ00467502 - (Closed) - State of the Shielded Drive is not displayed using storcli command
SCGCQ00569935 - (Closed) - PPC64 :: MR Liberator :: Storcli Version 1.09.01 is showing wrong Creation Date and Time in VD properties
SCGCQ00574287 - (Closed) - MR_Inv_6.3_PPC:Storcli- Storcli gives 'Segmentation fault' while retriving 'advanced software options' on SLES11 SP2 PPC64
SCGCQ00627672 - (Closed) - MR6.4_StorCLI: c0 show controller health is failing
SCGCQ00674131 - (Closed) - StorCLIO_1.09.09 : Not able to set subOEMid in Rhel 5.10 x64 bit.
SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
SCGCQ00787705 - (Closed) - CPLD - userCodeDefinition should be shown as part of /c0 show all command
SCGCQ00792233 - (Closed) - CPLD UPDATE : cpld upgradableCPLD support bit need to add under hardware configuration
SCGCQ00796227 - (Closed) - rlListPtr is not handled properly in failure case
SCGCQ00804680 - (Closed) - Out-of-bounds access and array delete misuse
SCGCQ00819603 - (Closed) - With command "/c0 start diag" duration should be an optional param.
SCGCQ00820392 - (Closed) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
SCGCQ00827192 - (Closed) - PD fail events are not logging into the file properly in EFI environment
SCGCQ00830435 - (Closed) - LDViewMirror is giving segmentation fault
SCGCQ00839321 - (Closed) - Storcli gives wrong error code with respect to FW state while converting JBOD to UG
SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show 
SCGCQ00471116 - (Closed) - Pcli: Pcli crashes while try to set securitykey for controller.
SCGCQ00493491 - (Closed) - Storcli /c0 show ASO fails and delay in displaying
SCGCQ00521999 - (Closed) - CSET: storelib header file checkin for the latest changes done by storelib - (SCGCQ00521999)
SCGCQ00523370 - (Closed) - StorCLI reports controller status as 'OK' when Arctrus controller(9361-8i) booted in safe mode
SCGCQ00792211 - (Closed) - supportDrvActivityLEDSetting supported bit need to be update in Supported adapater Operations
SCGCQ00793354 - (Closed) - Incorrect sizeof expression in dcmdprm
SCGCQ00804663 - (Closed) - Variable going out of scope without freeing which causes memory leak
SCGCQ00813314 - (Closed) - Not able add new VD in Drive Group
SCGCQ00830269 - (Closed) - storcli /call show all fails with "command invalid"
SCGCQ00835758 - (Closed) - Storcli shows caching is enabled on Source VD when CCVD is in offline state
SCGCQ00348911 - (Closed) - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354" on Flatwood Board
SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00518201 - (Closed) - MR6.2 : Storcli shows incorrect "Bus" information when "/c0 show all" is run
SCGCQ00564008 - (Closed) - StorCli: Segmantation fault appearing in storcli when issuing /c0/fall show
SCGCQ00622605 - (Closed) - CS2.0: Ctrl-R Domain Id is not showing in controller properties
SCGCQ00789402 - (Closed) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
SCGCQ00792205 - (Closed) - supportForceFlash needs to add under suported adapter operations
SCGCQ00795334 - (Closed) - Operands don't affect result in pddatamf.cpp causing wrong result
SCGCQ00811117 - (Closed) - LibMod changes for CTLR+R to read Disk Write Cache settings of PD.
SCGCQ00477037 - (Closed) - CLI reporting Large VD (56TB) size slightly smaller than other apps (by .001)
SCGCQ00603174 - (Closed) - /c0 set cc=conc command fails with iMR card.
SCGCQ00795342 - (Closed) - Unchecked return value in rmdatamf.cpp (getControllerStatus)
SCGCQ00801311 - (Closed) - MR_6.7_Storcli: Storcli reports wrong tmm and scap date of manufacture under scap properties in RHEL6.6 PPC64
SCGCQ00853185 - (Closed) - Storcli fails to dump lastoneday pdfailevents in a file.
SCGCQ00792085 - (Closed) - StorCLI :supportDisableImmediateIO adapter properties need to be added under show all command
SCGCQ00792234 - (Closed) - Firmware error code status MFI_STAT_SECURE_SYSTEM_PD_EXISTS needs to be update in code
SCGCQ00793361 - (Closed) - Non-array delete for objects in rmdatamf
SCGCQ00793363 - (Closed) - Resource leak in VdDataMf scanPartitions
SCGCQ00795336 - (Closed) - Explicit null dereferenced in vddatamf.cpp (getVdDetldInfo)
SCGCQ00804672 - (Resolved) - Non-array delete for objects: destructors will not be called for objects in the array leading to unexpected beh
SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applicaions
SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00818101 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
SCGCQ00829204 - (Implemented) - LibMods: Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
SCGCQ00726019 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
SCGCQ00755527 - (Closed) - Enable SED on JBOD
SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
SCGCQ00787923 - (Implemented) - OEL Support for SPARC
SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOB
SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on 12.12.0-0178
SCGCQ00818987 - (Closed) - LimMod changes related to CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
SCGCQ00828476 - (Closed) - Storcli Should display SAS Address N/A if its invalid and change Host interface type names from PCIX, PCIE to PCI-X, PCI-E
SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
SCGCQ00349599 - (Implemented) - Refer attached design doc
SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
SCGCQ00827663 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
SCGCQ00827665 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time res
SCGCQ00665081 - (Closed) - If any error that is returned as negative we return it s 0xFF from CLI to shell else FW returned error status will be returned to shell.
SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
SCGCQ00794841 - (Closed) - Functionality to extract field value from new API changes
SCGCQ00795150 - (Opened) - UDK Support for EFI
SCGCQ00816344 - (Implemented) - Utilities/Applications should not assume that expanders are enclosures as this is not always the case.
SCGCQ00817977 - (Closed) - Monitoring Drive performance and predictive failure
SCGCQ00817980 - (Closed) - Storcli: Monitoring Drive performance and predictive failure
SCGCQ00342399 - (Implemented) - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault a

Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.






SAS MegaRAID StorCLI
Release Date: 04/16/15


Version Numbers:	StorCLI
===============		===========			
Current Version		1.15.05
Previous Versoin	1.14.12


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00808112 - (Closed) - PDFwDownload with legacy syntax fails
SCGCQ00806973 - (Closed) - Not able to create VD using cfgcachecade add legacy syntax
SCGCQ00806493 - (Closed) - MR6.7:StorCLI throws error message as "Older Ver Image", when trying to Flash 4MB file from MR 6.7 Pack6 to Pack7
SCGCQ00804568 - (Closed) - Resource Leak : The system resource will not be reclaimed and reused, reducing the future availability of the resource
SCGCQ00804302 - (Closed) - Resource leak: Variable going out of scope leaks the storage it points to.
SCGCQ00803053 - (Closed) - storcli crashes on trying to flash the CPLD
SCGCQ00799098 - (Closed) - Smartpollinterval range to be changed from '1 to 65535' to '0 to 65535'
SCGCQ00797172 - (Closed) - Logically dead code in SwEvt.cpp
SCGCQ00797168 - (Closed) - Non-array delete for scalars SnpShtCp.cpp
SCGCQ00797143 - (Closed) - Resource Leak in LdRecn.cpp
SCGCQ00797088 - (Closed) - Structurally dead code in foreigncp.cpp (process_show)
SCGCQ00797085 - (Closed) - Explicit null dereferenced in ctcfpgcp.cpp (write_config_page)
SCGCQ00796128 - (Closed) - Memory leak due to Pdlist pointer
SCGCQ00795465 - (Closed) - Resource leak in cfgssccp.cpp(associateVDsToCachePool)
SCGCQ00795437 - (Closed) - Dereference before null check pdremfp.cpp
SCGCQ00795144 - (Closed) - Memory leak as UnCfgdVdOnFreeSpOnPd Class object is not freed
SCGCQ00795130 - (Closed) - storcli /c0 set cc doesnot have option to include all VD's.
SCGCQ00793707 - (Closed) - Set Supercap VPD information fails on PPC
SCGCQ00793396 - (Closed) - Comparing an array to null is not useful: "NULL != fspHdrList"
SCGCQ00793393 - (Closed) - Non-array delete for objects in trmlgcp.cpp
SCGCQ00793378 - (Closed) - Non-array delete for objects cfgechcp.cpp in associateVDsToCachePool
SCGCQ00793375 - (Closed) - Resource leak adpvpdcp.cpp in AdpSetVPD
SCGCQ00793372 - (Closed) - Non-array delete for objects adhwrcp.cpp handleReadSuboption
SCGCQ00790062 - (Closed) - "./storcli64 /c0 show cc" fails in RHEL 6.6 PPC64 with more than 64 VDs present
SCGCQ00790032 - (Closed) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
SCGCQ00789389 - (Closed) - autopdcache detailed help dose not have immediate option
SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
SCGCQ00725192 - (Closed) - Firmware Crash is hit while creating the Raid1 vd without drives selected
SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
SCGCQ00690355 - (Closed) - Storcli shows two controllers in the system though you have only one cotntroller in the system.
SCGCQ00653742 - (Closed) - Storlib header file checkin and make compatible changes in CLI code.
SCGCQ00644123 - (Closed) - "/cx/ex show phyerrorcounters" gives core dump on freeBSD 32 and 64 bit.
SCGCQ00579658 - (Closed) - PPC64 :: MR Liberator :: All commands of StorCli is failing with segmentation fault after creating a GlobalHotSpare
SCGCQ00574835 - (Closed) - MR_Inv_6.3_PPC:Storcli- Retreiving LDBBM info through storcli is failing on SLES11 SP2 PPC64
SCGCQ00568073 - (Closed) - Storclio_1.09.00:Fails to set SubOEMID on Solaris OS .
SCGCQ00518543 - (Closed) - PCLI Sparc(1.07.02):" Cli show all" command fails with error msg "Error! App exec failed in FW PCLIError! Internal".
SCGCQ00505771 - (Closed) - Wrong size of CacheCade VD is getting displayed after making one PD offline
SCGCQ00484560 - (Closed) - Try to create a Exclusive VD, but after creation it still shows as Shared VD.
SCGCQ00481474 - (Closed) - Some Numeric values in CLI o/p comes in Hex format
SCGCQ00479843 - (Closed) - Storcli internal errors should return with 1001, but its coming as -1
SCGCQ00355536 - (Closed) - MegaCli and StorCli can not manage both Liberato(and prior) and TB controllers in the same system under FreeBSD with the mf
SCGCQ00357948 - (Closed) - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
SCGCQ00359629 - (Closed) - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
SCGCQ00359998 - (Closed) - Code clean up in libmods and sysefi files are added
SCGCQ00360814 - (Closed) - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
SCGCQ00362216 - (Closed) - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
SCGCQ00362717 - (Closed) - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
SCGCQ00363455 - (Closed) - The legend for the PD List table exceeds 80 char limit.
SCGCQ00363522 - (Closed) - storcli query for displaying controller properties is showing status , as failure.
SCGCQ00364248 - (Closed) - StorCLI failed to delete a VD that is just created under Windows 2008
SCGCQ00364622 - (Closed) - Reports wrong diskgroup size while querying controller level properties
SCGCQ00364735 - (Closed) - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
SCGCQ00371445 - (Closed) - Vmware CLI fails to set the phy linkspeed
SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00381100 - (Closed) - MR: not able to create PRL11 using 96 drives.
SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00475583 - (Closed) - Storcli detecting the controller
SCGCQ00810266 - (Closed) - MR6.7-Misspellingof Minutes with storcli
SCGCQ00808109 - (Closed) - storcli -DpmStat -dsply hist physdrv[252:2] a0 fails
SCGCQ00804748 - (Closed) - Referring a pointer which was already freed.
SCGCQ00804578 - (Closed) - Variable not freed after allocating memory
SCGCQ00803754 - (Closed) - CCVD is creating with max array size where it has to be limited to 1TB
SCGCQ00803404 - (Closed) - After flashing expander firmware storcli is not displaying expected message .
SCGCQ00797137 - (Closed) - Dereference before null check in pdremfcp.cpp(validateExtractMaxLBAFromDriveCfgFile)
SCGCQ00797136 - (Closed) - Logically dead code in pddffprovcp.cpp(SendSTPCmd)
SCGCQ00797091 - (Closed) - Resource leak in ldaddcp.cpp(cfgOnNewArray)
SCGCQ00797087 - (Closed) - Use after free in expandvdcp.cpp (process_show)
SCGCQ00795892 - (Closed) - Memory leak as the pointer is not getting deleted when we return a failure.
SCGCQ00795434 - (Closed) - Dereference before null check in pddffdiagp.cpp
SCGCQ00795410 - (Closed) - No help provided for the command to uninstall storcli in ubuntu
SCGCQ00795147 - (Closed) - pdlist pointer is not getting deleted in failure case
SCGCQ00793729 - (Closed) - Some of the Design info parameters are missing for supercap
SCGCQ00793385 - (Closed) - Resource leak in encinfcp.cpp (process)
SCGCQ00793381 - (Closed) - Non-array delete for objects in deqlgcp.cpp (process)
SCGCQ00793379 - (Closed) - Resource leak in cfgssccp.cpp
SCGCQ00793373 - (Closed) - Array delete misuse - pdrmps.cpp
SCGCQ00790043 - (Closed) - "./storcli64 /c0 flasherase " fails in RHEL 6.6 PPC64
SCGCQ00789416 - (Closed) - StorCLI Code removal for removed ASD feilds in mr.h
SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
SCGCQ00649962 - (Closed) - Cannot create a VD smaller than 800MB with 4K drives
SCGCQ00649324 - (Closed) - MR6.4_StorCLI_240VD: StorCLI crashes on issuing /c1 set cc=conc delay=10 starttime=2014/12/12 12 excludevd=0
SCGCQ00644545 - (Closed) - storecli reports wrong size on 3000MB VD
SCGCQ00567761 - (Closed) - MR Liberator : PPC SERVERGY Server : MonTask: line 541 in file ../../raid/raidpci.c
SCGCQ00504585 - (Closed) - Some sparc structures missing for storcli.
SCGCQ00503981 - (Closed) - Command "./Storcli /call/eall/sx set offline" fails with ERRcode1001 and ERRmsg drive not found.
SCGCQ00490620 - (Closed) - Unable to insert a drive after setting a drive as 'Missing' .
SCGCQ00360040 - (Closed) - Storcli is returning error with show
SCGCQ00362070 - (Closed) - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
SCGCQ00362421 - (Closed) - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit
SCGCQ00364097 - (Closed) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00365632 - (Closed) - PCI Info for FreeBSD needs to be indicated as "N/A"
SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00378135 - (Closed) - portings of AdpRestart command
SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00424978 - (Closed) - MR6.1 Is VD Emulated=Yes when emulationType=1
SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00653672 - (Closed) - MR6.4: Storcli show command does not display all the controllers plugged into the server
SCGCQ00804712 - (Closed) - Resource leak - The system resource will not be reclaimed and reused.
SCGCQ00804666 - (Closed) - Variable not freed after allocating memory
SCGCQ00804583 - (Closed) - Resource leak in objects in Storcli: Constructor allocates memory but destructor does not free it.
SCGCQ00800414 - (Closed) - Coverity 13595 Unchecked return value
SCGCQ00800403 - (Closed) - Removing logically dead code performing actions that cannot occur
SCGCQ00795463 - (Closed) - Operands don't affect result in addevscp.cpp (setHSP)
SCGCQ00795439 - (Closed) - Dereference before null check in cfgsscdp.cpp
SCGCQ00794039 - (Closed) - Explicit null dereferenced (FORWARD_NULL) assign_zero: Assigning: "drvListPtr" = 0.
SCGCQ00793371 - (Closed) - Non-array delete for objects in adalogcp.cpp
SCGCQ00790050 - (Closed) - "./storcli64 /c0 show all page" shows "cachevault flash size = 8.0 ZB
SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
SCGCQ00729691 - (Closed) - MR6.5alpha:Segmentation fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
SCGCQ00695070 - (Closed) - storcli /c0 show all is not displaying "support vd hide" and "support HOQrebuild" feilds and legends are not displayed for HD
SCGCQ00674969 - (Closed) - Storcli doesn't show SN of Samsung SSD 200/400/800 in SWRAID version 1.32
SCGCQ00674023 - (Closed) - MR_6.4_StorCli_EFI: Storcli.efi crashes for iMR card.
SCGCQ00645195 - (Closed) - Storcli : unable to set patrol read delay
SCGCQ00609942 - (Closed) - storelib header file changes porting
SCGCQ00601775 - (Closed) - MR : on querying PR status, storcli hits segmentation fault
SCGCQ00581416 - (Closed) - PPC64 :: MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
SCGCQ00572800 - (Closed) - MR_Inv_6.3_PPC:Storcli-WWN is showing blank for SAS PDs on SLES11 SP2 PPC64
SCGCQ00529763 - (Closed) - Some characters missing while querying for VD properties with having 64 VD's on a controller.
SCGCQ00518579 - (Closed) - Unable to make R10 through Ctrl R using 4k drives
SCGCQ00499067 - (Closed) - Storcli reports VD Type as "Rec1" during reconstruction on SPARC.
SCGCQ00475815 - (Closed) - debug prints are present when issuing /co/eall show
SCGCQ00357263 - (Closed) - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
SCGCQ00366000 - (Closed) - Storcli displays incomplete serial number for some SSDs
SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite IBM Flatwood controller having power saving option completely disabled.
SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
SCGCQ00475562 - (Resolved) - Storcli - DFF firmware download fails with config ID mismatch on ESXi5.1
SCGCQ00807557 - (Closed) - Segmentation fault observed while trying to set JBOD as boot drive through legacy command in UBUNTU 14.10.
SCGCQ00804768 - (Closed) - Mesgptr is not getting deleted.
SCGCQ00804713 - (Closed) - LdTargetIdList is not getting freed in failure case
SCGCQ00796126 - (Closed) - fixing memory leak in bbu class
SCGCQ00793627 - (Closed) - Set autopdcache fails in PPC
SCGCQ00793394 - (Closed) - Non-array delete for objects in ttylogcp.cpp
SCGCQ00793386 - (Closed) - Non-array delete for objects in pdonlncp.cpp - (pdGetNissing)
SCGCQ00787431 - (Closed) - Dimmerswitch settings different in ctrl+r and storcli
SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
SCGCQ00674131 - (Closed) - StorCLIO_1.09.09 : Not able to set subOEMid in Rhel 5.10 x64 bit.
SCGCQ00627672 - (Closed) - MR6.4_StorCLI: c0 show controller health is failing
SCGCQ00574287 - (Closed) - MR_Inv_6.3_PPC:Storcli- Storcli gives 'Segmentation fault' while retriving 'advanced software options' on SLES11 SP2 PPC64
SCGCQ00569935 - (Closed) - PPC64 :: MR Liberator :: Storcli Version 1.09.01 is showing wrong Creation Date and Time in VD properties
SCGCQ00357913 - (Closed) - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
SCGCQ00360745 - (Closed) - StorCLI does not provide command to set HSM or HCOE SCGCQ0035866
SCGCQ00364332 - (Closed) - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00365950 - (Closed) - StorCLI cannot displays information for controller in Safe mode
SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00384644 - (Closed) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00465956 - (Closed) - No of blocks displayed for a VD remains same for all VD sizes.
SCGCQ00467502 - (Closed) - State of the Shielded Drive is not displayed using storcli command
SCGCQ00810638 - (Closed) - Added the condition to check the raid level and fail it if the drives given are lesser than the needed drives
SCGCQ00797139 - (Closed) - Structurally dead code in prfmoncp.cpp(process)
SCGCQ00797090 - (Closed) - Resource leak in ldaddcp.cpp(associateVDsToCachePool)
SCGCQ00793360 - (Closed) - Unchecked return value in appverp.cpp
SCGCQ00790022 - (Closed) - ./storcli64 /c0 show pr gives segmentation fault on PPC with more than 64 VDs
SCGCQ00523370 - (Closed) - StorCLI reports controller status as 'OK' when Arctrus controller(9361-8i) booted in safe mode
SCGCQ00521999 - (Closed) - CSET: storelib header file checkin for the latest changes done by storelib - (SCGCQ00521999)
SCGCQ00493491 - (Closed) - Storcli /c0 show ASO fails and delay in displaying .
SCGCQ00471116 - (Closed) - Pcli: Pcli crashes while try to set securitykey for controller.
SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show all.
SCGCQ00348911 - (Closed) - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
SCGCQ00804725 - (Closed) - userPdListPtr is not handled properly in failure case
SCGCQ00804682 - (Closed) - Resource Leak : This could cause an immediate crash or incorrect values might be read subsequently resulting in incorrect com
SCGCQ00800228 - (Closed) - Out of bounds access which can cause memory corruptions
SCGCQ00797165 - (Closed) - Non-array delete for scalars ShwSumCp.cpp
SCGCQ00622605 - (Closed) - CS2.0: Ctrl-R Domain Id is not showing in controller properties
SCGCQ00564008 - (Closed) - StorCli: Segmantation fault appearing in storcli when issuing /c0/fall show
SCGCQ00518201 - (Closed) - MR6.2 : Storcli shows incorrect "Bus" information when "/c0 show all" is run
SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354" on Flatwood Board
SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00793689 - (Closed) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
SCGCQ00603174 - (Closed) - /c0 set cc=conc command fails with iMR card.
SCGCQ00477037 - (Closed) - CLI reporting Large VD (56TB) size slightly smaller than other apps 
SCGCQ00796453 - (Implemented) - MR 6.7 - If execute delete CCVD force, StorCLI throws error code 0x3 MFI_STAT message but FW throws a proper message
SCGCQ00781004 - (Implemented) - Write-back caching support for non-RAID disks
SCGCQ00780967 - (Implemented) - Mechanism to set disk write cache on non-RAID disks - to enable / disable
SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applications
SCGCQ00790434 - (Closed) - Added a message to wait for some time after expander FW flash is success.
SCGCQ00787963 - (Implemented) - Address BBU/Supercap inconsistent Behavior across HSW apps.
SCGCQ00755527 - (Closed) - Enable SED on JBOD
SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
SCGCQ00787940 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00762265 - (Implemented) - Online Capacity Expansion by adding spans to RAID 10.
SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on 12.12.0-0178
SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
SCGCQ00349599 - (Implemented) - Refer attached design doc
SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
SCGCQ00796453 - (Implemented) - MR 6.7 - If execute delete CCVD force, StorCLI throws error code 0x3 MFI_STAT message but FW throws a proper message
SCGCQ00781004 - (Implemented) - Write-back caching support for non-RAID disks
SCGCQ00780967 - (Implemented) - Mechanism to set disk write cache on non-RAID disks - to enable / disable
SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
SCGCQ00685010 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00685007 - (Closed) - Added the library functions for the new MR API bits and LD operations.
SCGCQ00632240 - (Implemented) - SED/FDE changes for storcli Synchro
SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applications
SCGCQ00790434 - (Closed) - Added a message to wait for some time after expander FW flash is success.
SCGCQ00787963 - (Implemented) - Address BBU/Supercap inconsistent Behavior across HSW apps.
SCGCQ00755527 - (Closed) - Enable SED on JBOD
SCGCQ00642230 - (Closed) - Allow VMWARE version of STORCLI cannot be run from any directory
SCGCQ00564477 - (Implemented) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
SCGCQ00525321 - (Closed) - Implemented the diag results to print on console
SCGCQ00787940 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00558815 - (Closed) - MR 4.12: Big endian architecture support for MR Linux driver and StorCli
SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00762265 - (Implemented) - Online Capacity Expansion by adding spans to RAID 10.
SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on 12.12.0-0178
SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00621287 - (Closed) - STORCLI will support MR controller management without UEFI BootServiceDriver Driver and also has retain functionality of existing see- adapter-through-driver functionality.
SCGCQ00564474 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
SCGCQ00333209 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
SCGCQ00632051 - (Closed) - Added the OEM-NEC check for getting default disk-cache policy in Libmods as Disable.
SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
SCGCQ00349599 - (Implemented) - Refer attached design doc
SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
SCGCQ00467863 - (Implemented) - ASD- StorCLI - Libmod changes to support PD caching.
SCGCQ00693042 - (Implemented) - Complete 240VD support for utilities
SCGCQ00665081 - (Closed) - If any error that is returned as negative we return it s 0xFF from CLI to shell else FW returned error status will be returned to shell.
SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time reset
SCGCQ00436228 - (Opened) -
SCGCQ00342399 - (Implemented) - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault api
SCGCQ00518387 - (Port_Complete) - Storcli(1.07.01): Serial number is not displayed for Seagnus(9361-8i) card in RHEL 6.4 32 bit operating system.
SCGCQ00579103 - (Port_Complete) - Added the code to add the VD when there are missing drives on the array.
SCGCQ00602371 - (Active) - Need to display controller memory in Control-R
SCGCQ00758707 - (Port_Complete) - MR6.5_storCLI: VD property" Exposure to OS" equals to yes even after hidding the Virtual Drive.
SCGCQ00758750 - (Active) - Libmods changes for defect SCGCQ00726485: Commands for unintended controller during OCR.
SCGCQ00778747 - (Port_Complete) - Storcli get adpbootdrive legacy syntax fails
SCGCQ00614802 - (Port_Complete) - ASD- StorCLI- Libmod related changes for porting Virtual cache feature
SCGCQ00660804 - (Port_Complete) - Libmod changes for ER:SCGCQ00658772
SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
SCGCQ00758689 - (Active) - Libmods: SES Management Suspend Mode for Expanders
SCGCQ00766164 - (Port_Complete) - Displaying entire 8-byte HDD drive firmware version.
SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
SCGCQ00468257 - (Port_Complete) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00558869 - (Port_Complete) - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=<value>
SCGCQ00578945 - (Port_Complete) - Driver version is displayed as blank for Vmware split driver in CLI 1.08.01.
SCGCQ00653736 - (Port_Complete) - EnhancementRequest SCGCQ00650090: Add disable/enable BGI option in create VD dialog to CTRL-R
SCGCQ00688356 - (Port_Complete) - CTRL-R- Max config- Unable to create Raid10 VD using 192 Physical drives.
SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
SCGCQ00738979 - (Port_Complete) - Implemented the storcli command to print the smart data of SATA drives.
SCGCQ00469194 - (Port_Complete) - Aligning with FW for strip calculation for 4K drives(LIBMOD)
SCGCQ00498804 - (Port_Complete) - Unable to set PI to on/off .
SCGCQ00616621 - (Port_Complete) - Libmods changes for OP and Remanufacture NMR1.8
SCGCQ00678664 - (Port_Complete) - Libmod changes for defect SCGCQ00666029
SCGCQ00687252 - (Port_Complete) - Set MFC data using ini file fails for controller
SCGCQ00736025 - (Active) - MR6.5_RHEL5.10 : StorCLI crashing in *** glibc detected *** on trying to clear configuration on RHEL 5.10
SCGCQ00758122 - (Port_Complete) - Libmods: Display of CacheVault Flash Memory size
SCGCQ00793742 - (Port_Complete) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
SCGCQ00469169 - (Port_Complete) - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00477845 - (Port_Complete) - Checking in tab changes
SCGCQ00498784 - (Port_Complete) - RAID type is displayed as RAID0 for R5 VD on executing command "cli /fall show all" and "cli /fall import preview"
SCGCQ00643707 - (Port_Complete) - Perccli crashes on displaying controller information when there is a foreign config.
SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
SCGCQ00788882 - (Port_Complete) - MegaRAID CPLD update improvements
SCGCQ00790078 - (Port_Complete) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00437065 - (Port_Complete) - Driver Version is not shown in PercCli
SCGCQ00595789 - (Port_Complete) - StorcliF Application Error when running AdpDiags in WinPE
SCGCQ00610099 - (Port_Complete) - implemented the below commands for supporting limitsatato3G.
SCGCQ00631408 - (Port_Complete) - Added the library calls for supporting the personality mgmt.
SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
SCGCQ00756644 - (Active) - StorCLI : BBB Phase 1 - 128k threshold plus CLI enable/disable
SCGCQ00797738 - (Port_Complete) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00468241 - (Port_Complete) - Slow to create VD in HA Linux
SCGCQ00498801 - (Port_Complete) - Unable to create cachecade VD with WT property .
SCGCQ00578944 - (Port_Complete) - Wrong driver name is displayed for Vmware split driver in CLI 1.08.01.
SCGCQ00692501 - (Port_Complete) - Firmware crash (TLB) seen during removal of SAS cable form enclosure connected in multipath.
SCGCQ00789404 - (Port_Complete) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
SCGCQ00794454 - (Port_Complete) - Dimmerswitch settings different in ctrl+r and storcli
SCGCQ00576457 - (Port_Complete) - Multi CC cannot running concurrent even the setting is Concurrent
SCGCQ00589544 - (Port_Complete) - storcli incorrectly handle set SOE/stoponerror and set with opposite value
SCGCQ00518387 - (Port_Complete) - Storcli(1.07.01): Serial number is not displayed for Seagnus(9361-8i) card in RHEL 6.4 32 bit operating system.
SCGCQ00579103 - (Port_Complete) - Added the code to add the VD when there are missing drives on the array.
SCGCQ00602371 - (Active) - Need to display controller memory in Control-R
SCGCQ00758707 - (Port_Complete) - MR6.5_storCLI: VD property" Exposure to OS" equals to yes even after hidding the Virtual Drive.
SCGCQ00758750 - (Active) - Libmods changes for defect SCGCQ00726485: Commands for unintended controller during OCR.
SCGCQ00778747 - (Port_Complete) - Storcli get adpbootdrive legacy syntax fails
SCGCQ00614802 - (Port_Complete) - ASD- StorCLI- Libmod related changes for porting Virtual cache feature
SCGCQ00660804 - (Port_Complete) - Libmod changes for ER:SCGCQ00658772
SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
SCGCQ00758689 - (Active) - Libmods: SES Management Suspend Mode for Expanders
SCGCQ00766164 - (Port_Complete) - Displaying entire 8-byte HDD drive firmware version.
SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
SCGCQ00468257 - (Port_Complete) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00558869 - (Port_Complete) - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=<value>
SCGCQ00578945 - (Port_Complete) - Driver version is displayed as blank for Vmware split driver in PercCLI 1.08.01.
SCGCQ00653736 - (Port_Complete) - EnhancementRequest SCGCQ00650090: Add disable/enable BGI option in create VD dialog to CTRL-R
SCGCQ00688356 - (Port_Complete) - CTRL-R- Max config- Unable to create Raid10 VD using 192 Physical drives.
SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
SCGCQ00738979 - (Port_Complete) - Implemented the storcli command to print the smart data of SATA drives.
SCGCQ00469194 - (Port_Complete) - Aligning with FW for strip calculation for 4K drives(LIBMOD)
SCGCQ00498804 - (Port_Complete) - Unable to set PI to on/off .
SCGCQ00616621 - (Port_Complete) - Libmods changes for OP and Remanufacture NMR1.8
SCGCQ00678664 - (Port_Complete) - Libmod changes for defect SCGCQ00666029
SCGCQ00687252 - (Port_Complete) - Set MFC data using ini file fails for Softlayer controller
SCGCQ00736025 - (Active) - MR6.5_RHEL5.10 : StorCLI crashing in *** glibc detected *** on trying to clear configuration on RHEL 5.10
SCGCQ00758122 - (Port_Complete) - Libmods: Display of CacheVault Flash Memory size
SCGCQ00793742 - (Port_Complete) - Reading Supercap VPD information fails on RHEL 6.6 PPC64
SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
SCGCQ00469169 - (Port_Complete) - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00477845 - (Port_Complete) - Checking in tab changes
SCGCQ00498784 - (Port_Complete) - RAID type is displayed as RAID0 for R5 VD on executing command "cli /fall show all" and "cli /fall import preview"
SCGCQ00643707 - (Port_Complete) - Perccli crashes on displaying controller information when there is a foreign config.
SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
SCGCQ00788882 - (Port_Complete) - MegaRAID CPLD update improvements
SCGCQ00790078 - (Port_Complete) - "./storcli64 /c0 show eghs" fails on RHEL 6.6 PPC64
SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00437065 - (Port_Complete) - Driver Version is not shown in PercCli
SCGCQ00595789 - (Port_Complete) - StorcliF Application Error when running AdpDiags in WinPE
SCGCQ00610099 - (Port_Complete) - implemented the below commands for supporting limitsatato3G.
SCGCQ00631408 - (Port_Complete) - Added the library calls for supporting the personality mgmt.
SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
SCGCQ00756644 - (Active) - StorCLI : BBB Phase 1 - 128k threshold plus CLI enable/disable
SCGCQ00797738 - (Port_Complete) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00468241 - (Port_Complete) - Slow to create VD in HA Linux
SCGCQ00498801 - (Port_Complete) - Unable to create cachecade VD with WT property .
SCGCQ00578944 - (Port_Complete) - Wrong driver name is displayed for Vmware split driver in PercCLI 1.08.01.
SCGCQ00692501 - (Port_Complete) - Firmware crash (TLB) seen during removal of SAS cable form enclosure connected in multipath.
SCGCQ00789404 - (Port_Complete) - Remove the code related to enableVCor feild this was used for ASD and now it is not used any more.
SCGCQ00794454 - (Port_Complete) - Dimmerswitch settings different in ctrl+r and storcli
SCGCQ00576457 - (Port_Complete) - Multi CC cannot running concurrent even the setting is Concurrent
SCGCQ00589544 - (Port_Complete) - storcli incorrectly handle set SOE/stoponerror and set with opposite value
SCGCQ00593831 - (Port_Not_Required) - Inconsistency LDBBM status shown in storcli.
SCGCQ00611867 - (Port_Complete) - Implemented the commands for ThermalPoll interval for SSD and HDD
SCGCQ00647256 - (Port_Complete) - ASD- MR 6.4 - NytroXD compilation related fix
SCGCQ00789418 - (Port_Complete) - StorCLI Code removal for removed ASD feilds in mr.h
SCGCQ00790077 - (Port_Complete) - "./storcli64 /c0 flasherase " fails in RHEL 6.6 PPC64


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.




SAS MegaRAID StorCLI
Release Date: 01/14/15


Version Numbers:	StorCLI
===============		===========			
Current Version		1.14.12
Previous Versoin	1.13.06


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00696870 (ENHREQ) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00755055 (DFCT) - Not able to flash Firware
SCGCQ00757356 (DFCT) - Show cc (ExcludeVD property) results in memory overwrite with 240VD support.
SCGCQ00757358 (DFCT) - Add adapterOperation support details in /c0 show all for cachebypassMode.
SCGCQ00758079 (DFCT) - MR 6.6 Prealpha:Incorrect Storcli version is displayed for MR 6.6 FreeBSD binary.
SCGCQ00758739 (DFCT) - StorCLI while executing SED command the syntax fails with unsupported token
SCGCQ00758756 (DFCT) - Imporper detailed help command discription for set security JBOD command
SCGCQ00757497 (ENHREQ) - LD Deletion stalling all IOs on 12.12.0-0178
SCGCQ00725192 (DFCT) - H330: Firmware Crash is hit while creating the Raid1 vd without drives selected
SCGCQ00730505 (DFCT) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
SCGCQ00752000 (DFCT) - In Windows and Linux only controller grouping is working but not sorting
SCGCQ00755063 (DFCT) - Add support bits for uneven-span and SSHA support
SCGCQ00756647 (DFCT) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
SCGCQ00757755 (DFCT) - MR6.6_StorCLI: Displaying"BBU Not Present" for Cache vault in iMR Fury Controller
SCGCQ00758920 (DFCT) - "Storcli.exe has stopped working" when issuing command to see controller badblocks.
SCGCQ00758924 (DFCT) - Exception with command /co show badblocks or "storcli /cx flasherase"
SCGCQ00759178 (DFCT) - SupportMaxRate SATA is not listed in PD allowed operations.
SCGCQ00759181 (DFCT) - Add adapterOperation support details in /c0 show all for Emulationtype.
SCGCQ00759183 (DFCT) - SED adapterOperation detailed is not shown in detailed show controller properties
SCGCQ00759187 (DFCT) - Boot Volume details is shown in Megacli but not with storcli.
SCGCQ00759213 (DFCT) - Unused errors present in foreign command processor
SCGCQ00759218 (DFCT) - Memset is used only for 4 bytes where it has to be reset for the size of buffer we create.
SCGCQ00759290 (DFCT) - SSM-FLASh drives property is displayed for regular drives.
SCGCQ00759862 (DFCT) - OEMID is coming as "Unknown" for /c0 show all
SCGCQ00759959 (DFCT) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
SCGCQ00759969 (DFCT) - Adapters are not listed in sorted order.
SCGCQ00760214 (DFCT) - /c0 show health all command does not show health for all drives
SCGCQ00760215 (DFCT) - show health command for drives is failing with error code 61
SCGCQ00760255 (DFCT) - Storcli_Patch_6.4 : Detailed help file is not generating for MFG
SCGCQ00760385 (DFCT) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
SCGCQ00760398 (DFCT) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
SCGCQ00760752 (DFCT) - /c0 show all does not list hwCfg information as compared to MegaCLI.
SCGCQ00760757 (DFCT) - add vd help is exceeding 80 character per line limit.
SCGCQ00761937 (DFCT) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
SCGCQ00762663 (DFCT) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
SCGCQ00763998 (DFCT) - Help missing for set sesmonitoring command
SCGCQ00764636 (DFCT) - StorCLI:Vd delete discardcache option for delete virtual drive should not support for Liberator & TB
SCGCQ00764658 (DFCT) - StorCLI /c0 show all command does not reflect the discard vd delete filed
SCGCQ00764794 (DFCT) - storcli crash when trying to import 240+64 vd at once
SCGCQ00765712 (DFCT) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
SCGCQ00765714 (DFCT) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
SCGCQ00765759 (DFCT) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
SCGCQ00766153 (DFCT) - BBMT entries corrected and uncorrected error counters are rounding off after max is reached.
SCGCQ00766154 (DFCT) - BadBlock count displayed with below commands are rounding off after max is reached.
SCGCQ00767040 (DFCT) - help content is wrong for command /c0 set pcilinspeed
SCGCQ00767061 (DFCT) - MBOX values for set pcilinkspeed are not aligned with MR API.
SCGCQ00767128 (DFCT) -
SCGCQ00767868 (DFCT) - StorCLI: Detailed Help for coercion command should have the description for thier Value as [ 0, 1 , 2]
SCGCQ00758101 (DFCT) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
SCGCQ00758770 (DFCT) - FW breaks in iMR when excluding VD's from CC
SCGCQ00723935 (DFCT) - Enclosure connector name not displaying properly
SCGCQ00749743 (DFCT) - Syncro SSHA : StorCLI /c0 show loadbalancemode show Load Balance OFF eventhought the fearure is ON
SCGCQ00770875 (DFCT) - MR 6.6 : Storcli for FreeBSD gives wrong version
SCGCQ00775217 (DFCT) - MR6.6_StorCLI: Showing BBU_Prop for cache vault instead of CacheVault_Prop for MR Controller card
SCGCQ00776897 (DFCT) - MR_6.6_StorCLI: Incorrectness in the Error message while deactivating the trial Key.
SCGCQ00777800 (DFCT) - storcli reports CCVD deleted even though its still under deletion process by FW
SCGCQ00779800 (DFCT) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
SCGCQ00780082 (DFCT) - Segmentation fault while trying to flash GasGauge file with "noverchk" switch.
SCGCQ00780773 (DFCT) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
SCGCQ00782882 (DFCT) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
SCGCQ00783289 (DFCT) - Firmware returns an error for DCMD MR_DCMD_SCAN_FOR_FOREIGN_CONFIGS, but storcli still goes ahead and fires import.
SCGCQ00783693 (DFCT) - Storcli running legacy Cli command for encinfo does not display the reults in the correct format
SCGCQ00787431 (DFCT) - Dimmerswitch settings different in ctrl+r and storcli
SCGCQ00794013 (DFCT) - too many bytes for ioctl, given [ffff], max [ff44]
SCGCQ00795836 (DFCT) - storcli /c0/eall show is giving segmentation on TB FW
SCGCQ00413396 (DFCT) - MR_Inv_6.1:StoreCLI- Reports CTRL+R is disabled (controller boot properties) but actually it is enabled
SCGCQ00797068 (DFCT) - SATA SSD Model string is truncated to 8 bytes in StorCLI /cx/sx/ex show all Device Attributes section
SCGCQ00797277 (DFCT) - SuperCap Capacitance from same system is showed inconsistent in -adpbbucmd and /cv show
SCGCQ00797726 (DFCT) - EFI Storcli is not show the PD information on Grantley server
 


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.



Component:
=========
SAS MegaRAID StorCLI
Release Date: 10/07/14


Version Numbers:	StorCLI
===============		===========			
Current Version		1.13.06
Previous Versoin	1.12.13


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
Linux-ppc
VMware
VMware MN
VMware MN-NDS
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
** Change list updated 10/07/14 -- no change to binaries **
SCGCQ00637551 - (Closed) - storcli.efi /c0 set migraterate is setting values even if the value is out of range
SCGCQ00698962 - (Closed) - Storcli /c0 show configautobalance display as OFF eventhought the feature is ON
SCGCQ00704313 - (Closed) - Legacy command for displaying LD information not working
SCGCQ00712596 - (Closed) - Storcli not able to show the pinned cache for 240 VDs
SCGCQ00713774 - (Closed) - STORCLI fail to execute Reconstruction with Degraded r6 VD
SCGCQ00717299 - (Closed) - Storecli expand array OCE Not possible, insufficient space, expand array to get the additional space
SCGCQ00725544 - (Closed) - Supercap properties reports wrong in storcli
SCGCQ00726485 - (Closed) - Commands for unintended controller during OCR, controller availability non transparent during OCR.
SCGCQ00735055 - (Closed) - Mismatch in the no of fields showing in /c0 show eventloginfo command according to the help file
SCGCQ00738817 - (Closed) - Incorrectness in auto patrol read starttime schedule, after changing the date.
SCGCQ00739945 - (Closed) - need to remove AWB option with creation of Cachecade vd from Helpfile
SCGCQ00740053 - (Closed) - storlci becomes unresponsive on trying to create multiple VD at a time.
SCGCQ00688530 - (Closed) - Not able to unhide individual VD's and DG hide/unhide does not work when one vd is hidden or unhidden in DG
SCGCQ00693466 - (Closed) - "Segmentation fault" Error message after executing Diagnostic cmd in storCLI and further execution resulting into PSOD
SCGCQ00705623 - (Closed) - Unsupported-command error on executing the command to set MFG data on controller in EFI shell .
SCGCQ00710783 - (Closed) - Detail-status is not required to be displayed for any command which is success
SCGCQ00720007 - (Closed) - Caching is not getting enabled on all SVD's at a time using StorCLI command
SCGCQ00735327 - (Closed) - using option 2 for join mirror performs the same operation as option 0
SCGCQ00686189 - (Closed) - Advance Software options is not displaying any value for MegaRAID CacheCade Pro2.0
SCGCQ00705593 - (Closed) - Command "show autopdcache " is not working correctly
SCGCQ00720446 - (Closed) - Show learn is not coming in Help File
SCGCQ00740182 - (Closed) - Showing incorrect VDs number after excluding the VDs from cc
SCGCQ00635336 - (Closed) - storcli /c0 set backplane mode=val if we give value 256 its taking as 0 and giving command as success.
SCGCQ00684010 - (Closed) - For iBBU battery typeiBBU09 the Next Learn time value is not correct in the output of storCLI command storcli64 /c0/bbu show
SCGCQ00687566 - (Closed) - Storcli error message is confusing
SCGCQ00691917 - (Closed) - on querying for backplane/controller PHY, errors get reported
SCGCQ00723767 - (Closed) - Incorrectness in Ctrl_Prop While getting output for /c0 show prcorrectunconfiguredareas
SCGCQ00693177 - (Closed) - Try to split mirror with /c0/dall split mirror, But split mirror is not happening on all vds.
SCGCQ00693187 - (Closed) - not giving detail status table for split mirror command.
SCGCQ00695247 - (Closed) - on querying the PHY info for the drive,storcli gives the junk data
SCGCQ00723938 - (Closed) - storcli is giving improper error message when i missed pdperarray while creating raid00
SCGCQ00731998 - (Closed) - StorCLI displaying unwanted fields for Non-Controller flash image.
SCGCQ00694027 - (Closed) - on querying the phy error counter for controller, storcli dosent fail the cmd
SCGCQ00709767 - (Closed) - 'disableCacheBypass' being treated inversely as 'cacheBypass'
SCGCQ00668543 - (Closed) - Not able to enable security on DG which are eligible for secured Drive Group
SCGCQ00705597 - (Closed) - Help is not present for "set autopdcache".
SCGCQ00711678 - (Closed) - Help of set consistency check showing special character
SCGCQ00716639 - (Closed) - Storcli TMM and SCAP info shows wrong numbers
SCGCQ00606760 - (Closed) - "set perfmode" accepting wrong inputs
SCGCQ00642227 - (Closed) - Implement Head of Queue drive rebuild for MegaRAID controllers
SCGCQ00656613 - (Closed) - Add ability to take a VD offline, bring back VD online 
SCGCQ00684957 - (Closed) - Need StorCLI-O for EFI
SCGCQ00707449 - (Implemented) - SSHA Licensing (PFK)
SCGCQ00709946 - (Active) - For iBBU battery typeiBBU09 the Next Learn time value is not correct in the output of storCLI command storcli64 /c0/bbu show
SCGCQ00719104 - (Port_Complete) - Missing learn cycle progress information in show learn command for cachevault.
SCGCQ00699266 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures
SCGCQ00722165 - (Active) - Liberator (SAS9260-8i) controllers indicate that the do not support JBOD mode
SCGCQ00690644 - (Port_Complete) - storcli.efi /c0 set migraterate is setting values even if the value is out of range
SCGCQ00732184 - (Active) - CLI command to access/modify Drive Activity LED
SCGCQ00731753 - (Active) - CLI command to access/modify Immediate IO
SCGCQ00690877 - (Port_Complete) - Advance Software options is not displaying any value for MegaRAID CacheCade Pro2.0
SCGCQ00691901 - (Port_Complete) - Not able to enable security on DG which are eligible for secured Drive Group


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.



Component:
=========
SAS MegaRAID StorCLI
Release Date: 08/08/14


Version Numbers:	StorCLI
===============		===========			
Current Version		1.12.13
Previous Versoin	1.09.13


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00617622 - (Closed) - Storcli- Gives Seg fault for './storcli /c0 show all' if a foreign Secured VD is present on the controller
SCGCQ00637551 - (Closed) - storcli.efi /c0 set migrate rate is setting values even if the value is out of range
SCGCQ00648409 - (Closed) - Value not popped up for successful completion of autopdcache=r0 command.
SCGCQ00649340 - (Closed) - Store add VD help should display R1 EC as supported raid level
SCGCQ00657399 - (Closed) - query for multiple enclosure properties is failing in storcli version-1.12.05
SCGCQ00659228 - (Closed) - storcli show file=***.rom displaying only firmware version
SCGCQ00668210 - (Closed) - Inconsistent scheduled learn time.
SCGCQ00672888 - (Closed) - Junk Characters observed in EFI storcli version : 1.12.07
SCGCQ00678562 - (Closed) - the phy number dosent come properly on querying the phy error counter
SCGCQ00606774 - (Closed) - command "set patrolread delay" showing negative time delay
SCGCQ00622402 - (Closed) - Changing the MR_MFC_DEFAULTS->biosContinueOnError behavior for StorCLI as per PDMs
SCGCQ00624834 - (Closed) - fw is not able create vd on all drive as r0 using storcli command without an option immediate
SCGCQ00624991 - (Closed) - there is no syntax for storcli64.exe /cx/ex show
SCGCQ00629272 - (Closed) - storcli /c0/v2-256 show results in segmentation fault
SCGCQ00644238 - (Closed) - improper statment for emulationType 0 in help & detailed help
SCGCQ00647260 - (Closed) - Storcli-1.12.03-a failure message is displayed for a successful operation
SCGCQ00653749 - (Closed) - "cfgcachecadedsply" command is not showing any CC VD details [when creating using EVS + CCVD]
SCGCQ00611955 - (Closed) - Update the storcli help file for this command ./stocli /c0 set eccbucketleakrate
SCGCQ00616901 - (Closed) - seeing junk characters for command "show termlog"
SCGCQ00626582 - (Resolved) - not able to create WB cachecade-VD
SCGCQ00627824 - (Closed) - -High Availability Properties alignment properly in adpallinfo detail.
SCGCQ00627826 - (Closed) - not able set emergency hotspare field in storcli
SCGCQ00646216 - (Closed) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog.
SCGCQ00647107 - (Closed) - LD emulation type set to 512e even though there only 512n drives are used during creation
SCGCQ00682484 - (Closed) - help file needs to be updated  for /cx/dx add mirror src=2
SCGCQ00684010 - (Closed) - For iBBU battery typeiBBU09 the Next Learn time value is not correct in the output of storCLI command storcli64 /c0/bbu show
SCGCQ00691917 - (Closed) - on querying for backplane/controller PHY, errors get reported
SCGCQ00645141 - (Closed) - Storcli reports VD state as offline if pinned cache is generated through CC VD removal
SCGCQ00646223 - (Closed) - adding mirror by setting src value to 0 will start rebuild on online drive
SCGCQ00649337 - (Closed) - Junk characters seen in storcli.efi –adpallinfo –a0 and storcli.efi /c0 show all
SCGCQ00695247 - (Closed) - on querying the PHY info for the drive,storcli gives the junk data
SCGCQ00666644 - (Closed) - using option 2 i.e ./storcli /c0/d0 add mirror src=2 give success but no operation is performed
SCGCQ00694027 - (Closed) - on querying the phy error counter for controller, storcli dosent fail the cmd
SCGCQ00615654 - (Closed) - Battery serial number is not coming properly as per termlogs
SCGCQ00627716 - (Closed) - unable to create VD using Storcli
SCGCQ00646344 - (Closed) - Overall Health of a controller is displayed as ERROR if there is no VD present.
SCGCQ00658427 - (Closed) - Need to handle the failed cases and junk/invalid image file scenario for storcli show file=<filename> command
SCGCQ00675388 - (Closed) - Storcli won't set cacheflushinterval to a value greater >= 10 using old megacli syntax
SCGCQ00670246 - (Closed) - add vd each type=r0 creation leads to Segmentation Fault
SCGCQ00678558 - (Closed) - the out put for phyerror counter goes beyound the limit of wordcount.
SCGCQ00678616 - (Closed) - Status of storcli controller show health command on card Failed
SCGCQ00621291 - (Closed) - Add storCLI command to read phy error counters (target, expander, controller)
SCGCQ00625566 - (Closed) - Add a feature to read and display the FW version from the .rom file for MegaRAID FW package
SCGCQ00634751 - (Closed) - Requirement for 512e implementation changes
SCGCQ00673086 - (Closed) - OAdd SSHA support to StorCLI
SCGCQ00610100 - (Port_Complete) - implemented the below commands for supporting limitsatato3G
SCGCQ00615523 - (Port_Complete) - doesn't have proper keyword to set the Dimmer switch property for DisableLDPS.
SCGCQ00631409 - (Port_Complete) - Add support bit check for flash-erase.
SCGCQ00654713 - (Port_Complete) - Help not displayed for diag when tagged with paniclog,smartlog and errorlog. - (SCGCQ00646216) --Updating review comments
SCGCQ00615522 - (Port_Complete) - displays 'Model' information incorrectly using PercCLI show
SCGCQ00626649 - (Port_Complete) - storcli /253-255 show gives segmentation fault.
SCGCQ00660446 - (Port_Complete) - WB CCVD is created eventhough WT is specified in Slice nytro Cache create option
SCGCQ00629199 - (Port_Complete) -  unable to create VD using Storcli
SCGCQ00615442 - (Port_Complete) - Porting OverProvisioning and Remanufacture to StorCli5.9 for NMR 1.8
SCGCQ00631330 - (Port_Complete) - set batterywarning command sets inproperly.
SCGCQ00631410 - (Port_Complete) - SSDThermalPollInterval value range starts from 1 not from 0
SCGCQ00614724 - (Port_Complete) - add VD nytrocache command displays a wrong error message if the CCVD is already present
SCGCQ00614177 - (Port_Complete) - StorCli Displays Incorrect Information for BatteryWarning versus MagaCli
SCGCQ00631411 - (Port_Complete) - Implemented the personality mgmt to set either HBA/RAID mode.
SCGCQ00670865 - (Port_Complete) - NMR1.8-Storcli shows success message on creating EC CCVD in WT mode
SCGCQ00691901 - (Port_Complete) - Not able to enable security on DG which are eligible for secured Drive Group
SCGCQ00690877 - (Port_Complete) - Advance Software options is not displaying any value for MegaRAID CacheCade Pro2.0
SCGCQ00611864 - (Port_Complete) - Porting megaSCu syntax to perccli for limitMaxRateSATAto3G
SCGCQ00611866 - (Port_Complete) - Implemented the commands for ThermalPoll interval for SSD and HDD
SCGCQ00615271 - (Port_Complete) - StorCLIF and StorCLIO - Porting VC features
SCGCQ00670863 - (Port_Complete) - Source VD association failed and Storcli application crashed while associating sourceVD to CCVD


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.





Component:
=========
SAS MegaRAID StorCLI
Release Date: 06/18/14


Version Numbers:	StorCLI
===============		===========			
Current Version		1.09.13
Previous Versoin	1.09.08


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00681802 - (Completed) - GG firmware update patch (GG firmware update support for following OSes: Windows, Linux, EFI, Ubuntu)
SCGCQ00681722 - (Closed) - storcli (megacli style) output difference in pdlist command
SCGCQ00682462 - (Closed) - Help file should be updated
SCGCQ00655156 - (Closed) - "storcli -AdpBIOS -BE -a0" no longer works
SCGCQ00682485 - (Closed) - status of the command id getting success with invalid GG file.
SCGCQ00682477 - (Closed) - option "Resetnow" should be blocked when flashing Gasguage
SCGCQ00698740 - (Closed) - Card with Empty module version doesn't update firmware if option "noverchk" is provided.
SCGCQ00683236 - (Closed) - In Rhel OS seeing wrong error code.
SCGCQ00658495 - (Port_Complete) - set batterywarning command sets inproperly.
SCGCQ00659836 - (Port_Complete) - StorCli Displays Incorrect Information for BatteryWarning versus MagaCli


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.




Component:
=========
SAS MegaRAID StorCLI
Release Date: 05/09/14


Version Numbers:	StorCLI
===============		===========			
Current Version		1.09.08
Previous Versoin	1.07.07


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00567786 - (Closed) - not able get enclosure status
SCGCQ00571823 - (Resolved) - Added a condition to check for no VDs in StrtDrCp
SCGCQ00573703 - (Closed) - Storcli shows wrong VD size for 4K VDs during foreign config import
SCGCQ00574165 - (Closed) - compare factorysettings is a factory command but works in storcli
SCGCQ00579423 - (Closed) - storcli - issung "storcli /c0/v256" command generating coredump segmentation fault
SCGCQ00600059 - (Closed) - Storcli creates configuration not using the OEM default value for Disk Cache Policy
SCGCQ00471826 - (Closed) - StorCli mbox value needs to be changed for the command "storcli /c0/bbu show gasgauge offset=1 numbytes=1"
SCGCQ00571832 - (Resolved) - Added a condition to check for no VDs
SCGCQ00574325 - (Closed) - Storcli 'show ds' command fails with message "LD Power saving is unsupported"
SCGCQ00598687 - (Closed) - for bbu command In properties schedule time is showing twice
SCGCQ00599761 - (Closed) - storcli /c0/e1,2,3 show is showing enclouser properties multiple times.
SCGCQ00622402 - (Closed) - Changing the MR_MFC_DEFAULTS->biosContinueOnError behavior for StorCLI as per PDMs
SCGCQ00484361 - (Closed) - Removed the option all from tokenizer as it is not supported for enclosure firmware download.
SCGCQ00563031 - (Closed) - Even though there are no drive groups, the command storcli /c0/dxxx set security=on is getting success
SCGCQ00565409 - (Closed) - while Rebuild was going on Storcli was allows to create a partial VD on the same drive group
SCGCQ00576233 - (Closed) -  ./storcli64 /c0/bbu set learnstarttime command is failing with segmentation fault
SCGCQ00595061 - (Closed) - Storcli shows wrong estimated time for a rebuilding drive.
SCGCQ00602401 - (Closed) - ./storcli64 /c0/e252 show status displays success message
SCGCQ00581367 - (Closed) - MOn issuing command Adpalilog -a0 the Storcli throws an error 0x0c on PPC server
SCGCQ00601834 - (Closed) - The SCAPVPD commands are described as BBU instead of CV.
SCGCQ00559492 - (Closed) - Storcli displays the cc estimated time left out for the vd's where the operation is not in progress
SCGCQ00573720 - (Closed) - Need to display skipped images by storcil package flashing
SCGCQ00574205 - (Closed) - ./storcli64 /c252 show is displaying controller information of 1st controller
SCGCQ00601212 - (Closed) - Detailed help for storcli /c0/v0 set hostaccess is not showing
SCGCQ00581982 - (Closed) - Difference in behaviour across windows and linux platform after flashing FW from storclif
SCGCQ00598488 - (Closed) - storcli /c256 show is showing O/P as wrong synatx.
SCGCQ00600176 - (Closed) - command "/c0/p8 show" causing cli crash in windows OS
SCGCQ00602926 - (Closed) - when we query help for set perfmode the range is not mentioned for maxflush lines & numiostoorder.
SCGCQ00606117 - (Closed) - storlib library depended Make file flags check in
SCGCQ00577682 - (Closed) - MR Liberator :: ./storcli64 /c0 show dequeuelog file command failing with segmentation fault
SCGCQ00588916 - (Resolved) - ./storcli64 /c0/sall show rebuild command shows success status
SCGCQ00598788 - (Closed) - "show termlog" command description is coming after displaying the logs.
SCGCQ00627716 - (Closed) - unable to create VD using Storcli
SCGCQ00553006 - (Closed) - Updated Help syntax for add vd w.r.t AWB
SCGCQ00572149 - (Closed) - Added the help changes for break and join mirror.
SCGCQ00601568 - (Closed) - nolog option is not working in MegaCLI
SCGCQ00526855 - (Implemented) - Link libstdc++ statically to Linux versiosn of Strcli, storclio and storclif
SCGCQ00602432 - (Closed) - Linux-ppc 32-bit minimum driver version supported by storcli 06.603.04.00.
SCGCQ00554055 - (Closed) - Big endian architecture support for MR Linux driver and StorCli
SCGCQ00555468 - (Closed) - Added OEM based help and displaying it.
SCGCQ00568855 - (Implemented) - Added new commands for join mirror
SCGCQ00550374 - (Implemented) - Added new commands for break mirror
SCGCQ00569363 - (Closed) - Implemented the below CS syncro commands
SCGCQ00564470 - (Implemented) - Request RAID CLI to display the Patrol Read Start Time
SCGCQ00523846 - (Implemented) - Storcli to flash 16 and 32 MB images
SCGCQ00593583 - (Port_Complete) - In Storcli, appropriate error description to be logged when FW flash is failed
SCGCQ00601765 - (Port_Complete) - Storcli shows wrong estimated time for a rebuilding drive.
SCGCQ00576453 - (Port_Complete) - Found storli will show incorrect Next starttime after changing CC from Automatic to OFF.
SCGCQ00592293 - (Port_Complete) - Unable to replace failed drive
SCGCQ00598800 - (Port_Not_Required) - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
SCGCQ00558870 - (Port_Complete) - Implemented the deviceExposure as a BIOS option to set /c0 set BIOS deviceExposure=n
SCGCQ00564130 - (Port_Complete) - Added a condition to check for number of drives.
SCGCQ00604174 - (Active) - BiosContinueOnError IssueWebBIOS for SAS9265-8i controller incorrectly reports "Pause on errors" instead of "Bypass Error"
SCGCQ00593384 - (Port_Complete) - SCSI bus reset while collecting TFF smart logs
SCGCQ00593417 - (Port_Complete) - 1.05.56 rpm installation failed saying "scriptlet failed, exit status 1"
SCGCQ00593572 - (Port_Complete) - TFF firmware upgrade succeeded with mode 7 on Eagle board
SCGCQ00567735 - (Port_Complete) - not showing DS3 enable properties.
SCGCQ00578982 - (Port_Complete) - and storclif mention "nytrocache" in help message not an OEM feature
SCGCQ00593226 - (Port_Complete) - When attempting to update DFF firmware, update fails with error "Failure 1001 failed to get ssd Controller type.
SCGCQ00593386 - (Port_Complete) - 'start format' command form stocli on unconfigured drive deletes all the vds configured
SCGCQ00598815 - (Port_Complete) - StorCLI adpalilog command crashes in Windows 2012 R2 Build 9600 - version 1.06.03 and version 1.03.46
SCGCQ00563046 - (Port_Complete) - storcli64.exe /c0/cv start learn option is not present
SCGCQ00575400 - (Port_Complete) - Getting segmentation fault when executed the command /c0 compare factorysettings file= file name
SCGCQ00555931 - (Port_Complete) - storclif 1.07.06 does not have memory scrub test available
SCGCQ00567476 - (Port_Complete) - getting segmentation fault when executed the command /c0 set factory file=filename
SCGCQ00578979 - (Port_Complete) - space present in command compare factorysettings between words factorysettings
SCGCQ00593402 - (Active) - Successful command execution depicted as a "failure" for the command: "add each vd type=r0"
SCGCQ00593571 - (Port_Complete) - Storcli doesn't provide "Description" in output when extract paniclog is issued on all the TFFs.
SCGCQ00593568 - (Active) - Storcli doesnot prompt the user to reboot the host after changing the link speed of a TFF.


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.





Component:
=========
SAS MegaRAID StorCLI
Release Date: 01/20/14


Version Numbers:	StorCLI
===============		===========			
Current Version		1.07.07
Previous Versoin	1.05.07


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00493418 - (Closed) - FW breaks to MegaMon on executing "Cli /eall/sall show all" command.
SCGCQ00501866 - (Closed) - Time Left is not show correctly by sparc storcli
SCGCQ00521869 - (Closed) - /call/eall show not providing details of enclosure connected to the second controller
SCGCQ00526799 - (Closed) - Not able to flash PD firmware of 4TB Drive using storcli
SCGCQ00485777 - (Closed) - FW breaks to Megamon, after creating 16 R0 VD's and on executing command "cli /vall show all" from PCLI.
SCGCQ00501376 - (Closed) - "/c0 show dequeuelog file=_____" command is not working in OS OEL_5.9
SCGCQ00503993 - (Closed) - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
SCGCQ00505348 - (Closed) - The help file for "/c0 start Diag duration=___" is missing
SCGCQ00503359 - (Closed) - Wrong PCLI version with junk charcters are displayed under GetControllerInfo.
SCGCQ00498965 - (Closed) - "/c0/bbu start learn" command starts battery learn cycle on supercap battery.
SCGCQ00518133 - (Closed) - LSI_MR Controllers fails to set "FACTORY SETTINGS"
SCGCQ00526503 - (Closed) - Flashing of FW in UEFI mode using storcli.efi is issuing File read error.
SCGCQ00501383 - (Closed) - "/c0 show dequeuelog file=_____" command is missing in main help file
SCGCQ00501414 - (Closed) - Online firmware update is not triggered on flashing FW
SCGCQ00524047 - (Closed) - Segmentation fault occures while converting binary to text file of DQlogs
SCGCQ00526385 - (Closed) - Unable to create cachecade VD with WT property .
SCGCQ00522666 - (Closed) - Command "cli /sall show all" 
SCGCQ00524755 - (Closed) - Storcli- Gives incomplete message while clearing config when CC VD is present on the controller
SCGCQ00493544 - (Closed) - "Error! App exec failed in FW PCLIError! Internal" is displayed on executing "Cli /eall/sall spindown" command with 25 drives.
SCGCQ00501437 - (Closed) - StorCLI - MR 6.2 StorCLI help syntax is wrong
SCGCQ00518372 - (Closed) - Displaying the Adapter health status in storcli show.
SCGCQ00501561 - (Closed) - Implemented the diag results to print on console
SCGCQ00484168 - (Closed) - Implemented the AWB for VD creations
SCGCQ00526393 - (Active) - Implementation of "MegaCli adpbbucmd schedulelearn [options.....] an" equivalent command in storcli
SCGCQ00304999 - (Closed) - SWR- Retrieval of controller information fails .
SCGCQ00305001 - (Closed) - storcli command- show DS displays wrong information for type4 and DS off
SCGCQ00307493 - (Closed) - (RW LSIP200233165) Storcli: Reocurance should be spelled as reoccurrence in controller show all properties for PR and CC
SCGCQ00307495 - (Closed) - Displaying the correct operating system for Windows 2012 Server
SCGCQ00308671 - (Closed) - StorCLI is not showing correct driver version in Solaris 11
SCGCQ00309347 - (Closed) - StorCli-SATA Drives "PRODUCT ID" its not showing properly.
SCGCQ00312089 - (Closed) - Storcli- Not able to perform erase operation on a PD on VMWare 4.1 update 2
SCGCQ00312319 - (Closed) - Storcli- Status of /pall set linkspeed is showing success eventhough the operation is failure on ESX 4.1 update 2
SCGCQ00314106 - (Closed) - Remove all negative error codes
SCGCQ00314585 - (Closed) - StorCli - Cache cade VD information page doesn't have any details for associated VDs.
SCGCQ00322316 - (Closed) - Defect: Storcli-Controller show/set help page in that last line execute with Storcli Directory.
SCGCQ00328184 - (Closed) - StorCLI2.0: "endCtlrPropUpdate failed 4" when changing the properties of patrolread
SCGCQ00335239 - (Closed) - Virtual Drive properties(stripe size and size) got changed when VD is degraded
SCGCQ00338301 - (Closed) - StorCLI : Not able to set BBU modes using legacy syntax in EFI Environment
SCGCQ00341488 - (Closed) - stocli_EFI- In paged view the next line after "press enter to continue " should be displayed in next line
SCGCQ00342056 - (Closed) - StorCLI - in command "./storcli show " 2 fields are not getting displayed ( 1. Host Name , 2. Operating System )
SCGCQ00342074 - (Closed) - storcli should not depend on MFC_FEATURES instead check the other bits which indicates whether a particular feature is supported
SCGCQ00342549 - (Closed) - spelling mistake of initialization in (background initialization)
SCGCQ00343721 - (Cloned_EnhReq) - Drive /c0/ex/sx Hot Spare Information, displays array info under Dedicated Drive Group(s) = 0, 1
SCGCQ00343907 - (Closed) - StorCLI_EFI: System halts while performing import preview with securitykey in EFI Environment
SCGCQ00345525 - (Closed) - On performing an "add vd" with size provided in TB a decimal value is truncated to whole number as input.
SCGCQ00349419 - (Closed) - storcli /c0 show all -----> driver version and driver name field is missing
SCGCQ00350744 - (Closed) - ./storcli /c0/dall show -----> In the drive group info the alignment for global hot spare drive is improper.
SCGCQ00352569 - (Closed) - Buffer overflow
SCGCQ00360745 - (Closed) - StorCLI does not provide command to set HSM or HCOE SCGCQ00358662
SCGCQ00362717 - (Closed) - storcli /c0/d0 show " in that legend missing for "Dgrd/pdgd/Onln/ofLn/Rbld"
SCGCQ00363522 - (Closed) - storcli query for displaying controller properties is showing status , as failure.
SCGCQ00364248 - (Closed) - StorCLI failed to delete a VD that is just created under Windows 2008
SCGCQ00364622 - (Closed) - Reports wrong diskgroup size while querying controller level properties
SCGCQ00381100 - (Closed) - MR: not able to create PRL11 using 96 drives.
SCGCQ00462959 - (Closed) - Slow to create VD in HA Linux
SCGCQ00464708 - (Closed) - Storcli display total number of VDs in a individual drive group properties.
SCGCQ00466519 - (Closed) - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
SCGCQ00467119 - (Closed) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00481532 - (Closed) - Msg comes for all /c0 show commands.
SCGCQ00305002 - (Closed) - Storcli:Unable to update PD Firmware using Storcli in Vmware 5.0
SCGCQ00310308 - (Closed) - Storcli -Format for Date/Time varies in show|show all controller properties .
SCGCQ00313759 - (Closed) - Storcli:Unable to create Cachecade VD in Windows 8
SCGCQ00314602 - (Closed) - StorCli - Cachecade VD information page should not display stripe size.
SCGCQ00316677 - (Closed) - Logical and Physical sector size must be hidden when 512E feature is not supported
SCGCQ00322262 - (Closed) - iMR_Inv:37 drives shown as unconfigured good in MegaCLI when "enable JBOD=0" in Ubuntu 12.04 32 bit OS
SCGCQ00324797 - (Closed) - Serial Number of controller is not displayed for some controllers.
SCGCQ00332212 - (Closed) - libsysfs custom implementation issue.
SCGCQ00341418 - (Closed) - In the command O/P of <./storcli /c0 show all>"Driver Name" and "Driver Version"are NOT matching with actual name and version
SCGCQ00342723 - (Closed) - It is displaying the driver version as driver name
SCGCQ00344992 - (Closed) - In the command O/P of <./storcli /c0 show all>, ErrMsg 255 Failed to get Bus Info is displayed
SCGCQ00348911 - (Closed) - Adapter 0: Failed to start SecureErase on Virtual Drive 0 in VMware_ESXi_5.1
SCGCQ00353679 - (Closed) - StorCli-"/c0/eall/sall show"in that need to be describe the GHS/Onln/Offln/F
SCGCQ00355536 - (Closed) - MegaCli and StorCli can not manage both Liberator (and prior) and TB controllers in the same system under FreeBSD with the mfi adn mrsas driver.
SCGCQ00357653 - (Closed) - Removing static memory allocation and allocating memory dynamically in function stricmp in file Cutils.cpp
SCGCQ00357913 - (Closed) - Update VD emulation feature in StorCLI Libmods module to sync with latest APIs.
SCGCQ00359998 - (Closed) - Code clean up in libmods and sysefi files are added
SCGCQ00360814 - (Closed) - StorCLI: Not able to set pr property includessds as onlymixed on Liberator cacheoffload controller
SCGCQ00362421 - (Closed) - StorCLI: Not able to detect Liberator Controller on FreeBSD 9.0(64-bit)
SCGCQ00364097 - (Closed) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00366000 - (Closed) - Storcli displays incomplete serial number for some SSDs
SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00469162 - (Closed) - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00476030 - (Closed) - while running I/O ,It's taking time to load the controller information.
SCGCQ00312928 - (Closed) - Storcli- Abbreviation of UID should be mentioned in the output for /cx/fall show all
SCGCQ00314122 - (Closed) - Missing characters in PD model display
SCGCQ00317649 - (Closed) - Defect: StorCli-VD state "Dgrd'' is changed in the description-''dgrd''
SCGCQ00326862 - (Closed) - FreeBSD support for MegaWare Cli
SCGCQ00338688 - (Closed) - Storcli spelling mistakes and typos
SCGCQ00343593 - (Closed) - Description for different Drive "State" like DHS, Ugood, Online need to be provided under Show Drive Information
SCGCQ00363455 - (Closed) - The legend for the PD List table exceeds 80 char limit.
SCGCQ00364735 - (Closed) - UEFI, the O/P of <storcli /c0 show all>"Current Controller Date/Time" & "Current System Date/time" are not in proper format
SCGCQ00371445 - (Closed) - Vmware CLI fails to set the phy linkspeed
SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
SCGCQ00460861 - (Closed) - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
SCGCQ00462885 - (Closed) - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00466038 - (Closed) - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
SCGCQ00466251 - (Closed) - HA : StorCLI crash when update drive firmware
SCGCQ00471042 - (Closed) - PCLI:Cant able to set securitykey for Controller and also VD name for VD(Takes as uppercharacter even if name given in lower)
SCGCQ00485270 - (Closed) - StorCLI- unsupported CV operations for SuperCap 'set' needs to be removed
SCGCQ00311990 - (Closed) - Removed unsupported property "Ra=Read Ahead Adaptive" from VD information.
SCGCQ00314114 - (Closed) - sector size of PDs are shown as 512 KB which is wrong.
SCGCQ00314128 - (Closed) - Add abbreviation description to all the PD states
SCGCQ00318435 - (Cloned_EnhReq) - Porting of 1.0 PRs to storcli phase 2.5 (Libmods)
SCGCQ00345372 - (Closed) - Storcli command "/cx show all" must display ROC temperature.
SCGCQ00359629 - (Closed) - In paged view the text " Press Enter to continue" should be changed to " Press any key to Continue"
SCGCQ00365950 - (Closed) - StorCLI cannot displays information for controller in Safe mode
SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00469179 - (Closed) - Aligning with FW for strip calculation for 4K drives
SCGCQ00337962 - (Closed) - StorCLI: not able to save events in txt file in EFI environment
SCGCQ00362216 - (Closed) - iMr_Fury_StorCli:4K Drive size shown wrong in Esxi4.1U3
SCGCQ00365632 - (Closed) - PCI Info for FreeBSD needs to be indicated as "N/A"
SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in SGI system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00485561 - (Closed) - storclio set and get vpd gives a wrong output in failure case.
SCGCQ00493690 - (Closed) - /var/tmp//installobaWVe/checkinstallrbaWVe: line 11: syntax error at line 22
SCGCQ00481039 - (Closed) - option -v doesn't work with preboot storcli
SCGCQ00311436 - (Closed) - Storcli-SWR- Controller serial number display is different in show/showall controller properties .
SCGCQ00360040 - (Closed) - Storcli is returning error with show
SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00470976 - (Closed) - Storcli shows irrelevant information about Nytro cache VD when user types "CfgCacheCadeDsply"
SCGCQ00484372 - (Closed) - Storcli:Help file modification required for command ''/cx set eghs''
SCGCQ00357263 - (Closed) - MegaCLI adpgetpciinfo returns a static Bus Number value "17d0"
SCGCQ00362070 - (Closed) - iMr_Fury_StorCLi:SectorSize show as "512KB" for 512Bytes drives
SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00424978 - (Closed) - Is VD Emulated=Yes when emulationType=1
SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show all.
SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
SCGCQ00471978 - (Closed) - Storcli does not show firmware version using Megacli syntax
SCGCQ00472000 - (Closed) - Storcli:"storcli /c0/v0 del help" does not show information on normal vd delete
SCGCQ00314119 - (Closed) - "Drive NCQ setting" field Removed
SCGCQ00357948 - (Closed) - StorCLI does not display drive information behind the Blackjack (Alta) interposer correctly
SCGCQ00384644 - (Closed) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00484230 - (Closed) - "Cli /ex/sx set offline" fails with errcd -1 and message enclosure ID not found.
SCGCQ00495121 - (Closed) - Unable to set pnpid using the ini file with captal letters mixed in the string
SCGCQ00330250 - (Closed) - StorCLI compliance with OSSRB recommendation
SCGCQ00342399 - (Implemented) - CSET: (Tbolt PR 211180) Punctured Block Logging Improvements
SCGCQ00329470 - (Closed) - Implemented the StorCLI commands to erase contents from NVCache
SCGCQ00488282 - (Implemented) - Add ability to change/program PCIDATA in StorClio (CLI for OEMs)
SCGCQ00501189 - (Implemented) - MWCLI. Add command /cX/vX locate
SCGCQ00323426 - (Implemented) - Porting of Vogel 1.0 PRs to storcli phase 2.5 [Libmods]
SCGCQ00349599 - (Implemented) - Refer attached design doc
SCGCQ00352120 - (Implemented) - MWCLI. Add HA support into storcli
SCGCQ00329469 - (Closed) - Implemented the StorCLI commands to scrub memory on controllers
SCGCQ00332606 - (Implemented) - Display Drive Model number, Serial Number and Firmware Revision as in MSM
SCGCQ00349548 - (Closed) - Uneven span support is added in StorCLI.
SCGCQ00351234 - (Implemented) - Provide a way to enable or disable 512E using Applications
SCGCQ00479543 - (Implemented) - MWCLI: Need MegaOEM for Solaris x86 and Solaris SPARC
SCGCQ00333213 - (Closed) - Implemented 128 drive support by using the new ENCL_INFO structures
SCGCQ00322837 - (Closed) - Printing multiple json objects from different controllers as a single Array
SCGCQ00332600 - (Implemented) - StorCLI compliance with OSSRB recommendation
SCGCQ00350668 - (Implemented) - Create Spanned R0 array (00) in StorCLI
SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault api
SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time reset
SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
SCGCQ00469192 - (Port_Complete) - Aligning with FW for strip calculation for 4K drives
SCGCQ00471590 - (Port_Complete) - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00504584 - (Port_Complete) - Command "./storcli /call/eall/sall show" fails for second controller with description drive not found.
SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00437065 - (Port_Complete) - Driver Version is not shown
SCGCQ00473065 - (Port_Complete) - StorCli_6.1: The SATA drive is dropped while creating a R1 vd using mix of SAS and SATA drives
SCGCQ00478786 - (Port_Complete) - (v 1.04.11) get a good return code (0) even when it failed
SCGCQ00471582 - (Port_Complete) - Storclio:Spelling mistake during execution of command 'compare factorysettings'
SCGCQ00475598 - (Port_Complete) - Storcli:4K -Wrong size updated after performing OCE on 4K Drives .
SCGCQ00475601 - (Port_Complete) - storcli crash while using the command /cx/vx expand size=xx expandarray
SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00481849 - (Port_Complete) - StorCLI- StorCLI reports wrong capacitance value for supercap FBU03
SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
SCGCQ00471048 - (Active) - HA : StorCLI crash when update drive firmware
SCGCQ00469390 - (Port_Complete) - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03


Installation Commands: 
=======================
Any OS specific instructions are noted in a readme file included in a folder in the zip file.
Refer to the MegaRAID SAS Software User's Guide for any additional StorCLI information.  The User Guide can be found in the MegaRAID Documentation section of www.lsi.com.




Component:
=========
SAS MegaRAID StorCLI
Release Date: 09/23/13


Version Numbers:	StorCLI
===============		===========			
Current Version		1.05.07
Previous Versoin	1.04.07


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris x86
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00009501 - (Closed) - MPI2_FW_IMAGE_HEADER is 16 bits too long
SCGCQ00183867 - (Closed) - MPI2: IO Unit Page 10 structure incorrect
SCGCQ00364332 - (Closed) - iMR_Inv_6.1:StoreCLI-StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00374732 - (Closed) - StorCLI cannot set "bypasserror" or "be"
SCGCQ00374733 - (Closed) - Storcli does not show 512 strip size in the online help
SCGCQ00378124 - (Closed) - Porting of AdpRestart Command
SCGCQ00379046 - (Closed) - MegaCLI help shows Storcli in generic help command
SCGCQ00379112 - (Closed) - storcli-legacy: The helpfile for "adpfwflash" needs to be updated for "NoVerChk"
SCGCQ00381383 - (Closed) - Storcli_Invader: "/c0 pause pr" Description message should be sync with command
SCGCQ00394588 - (Closed) - storcli only displays 1 vd when 7 present on DG view
SCGCQ00397280 - (Closed) - StorCli_MR:Need to modify the "DIMMER SWITCH" Help Description
SCGCQ00397877 - (Closed) - SWR: EFI:"Press any key to continue" displays twice.
SCGCQ00397893 - (Resolved) - SWR: EFI: Operating system details shows nothing.
SCGCQ00399897 - (Closed) - BBU GasGauge Status information should not get printed for TMMC
SCGCQ00400429 - (Closed) - Storcli help lists unsupported /Fx option for foreign commands
SCGCQ00406358 - (Closed) - CLI does not provide appropriate error message and error code when secure erase is not supported
SCGCQ00414300 - (Closed) - StorCli_6.0-The help file for "storcli /cx/fx " is missing.
SCGCQ00415814 - (Closed) - storcli only associates 38 out of 48 VDs
SCGCQ00418295 - (Closed) - size=0 VD is getting created with remaining free space, when a VD is present in Drive Group.
SCGCQ00421114 - (Closed) - Storcli/Storclif/storclio:Help file for Legacy commands displays mrcli instead storcli.
SCGCQ00421282 - (Closed) - StorCLIO : not able to get or set hwdevice information with storCLIO
SCGCQ00423757 - (Closed) - EFI: Storcli : Not able to get and set vpd information on TMM module or Supercap
SCGCQ00435852 - (Closed) - misspelled word in storcli.efi message
SCGCQ00437754 - (Closed) - Help syntax is not aligned with 80 char per line limits.
SCGCQ00449926 - (Closed) - Power Shell support for megacli syntax for windows _ Porting
SCGCQ00450496 - (Closed) - StorcliF : output for the command /c0 compare factorysettings is not in sync with the legacy output.
SCGCQ00456135 - (Closed) - Unable to create Cachecade VD by referring the syntax in Help file for ''add vd'' .
SCGCQ00462959 - (Closed) - Slow to create VD in HA Linux
SCGCQ00466519 - (Closed) - StorCLI_6.1:The help file for "/c0 compare securitykey h" is missing
SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374118 - (Closed) - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
SCGCQ00374979 - (Closed) - Storcli ld info command displays R10 vd Span Depth to 1.
SCGCQ00376643 - (Closed) - Fail to set/disable the Disk Cache Policy along with the vd creation.
SCGCQ00378135 - (Closed) - portings of AdpRestart command
SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00385101 - (Closed) - StorCli implementation of AdpRestart Command
SCGCQ00386429 - (Closed) - StorCLI help file shows /cx/dx show cachecade instead of /cx/dall show cachecade
SCGCQ00391731 - (Closed) - storcli displays message as firmware flash successfully completed even the flashing is failed.
SCGCQ00397014 - (Closed) - With one VD as foreign, StorCLI shows all VDs as foreign.
SCGCQ00397269 - (Closed) - StorCli_5.7: On SuperCap battery ''strat learn" operation is not allowed
SCGCQ00399002 - (Closed) - handleTokens(tokenListPtr);
SCGCQ00399387 - (Closed) - Not able to find range for Perf Mode value
SCGCQ00401663 - (Closed) - help text not working for the command set securitykey
SCGCQ00412827 - (Closed) - CV (CacheVault) does not support changing bbu mode but StorCLI show option to change bbu mode
SCGCQ00417435 - (Closed) - StorCLIF : the command /cx get hwdevice fails to get VPD information.
SCGCQ00417973 - (Closed) - Storclio/Storclif-Detailed help for the command start diag required .
SCGCQ00423781 - (Closed) - StorCLIF : getting wrong values for get gas gauge information.
SCGCQ00441696 - (Closed) - StoreCLI- Inconsistent behavior across different application when creating cachecade VD
SCGCQ00466251 - (Closed) - HA : StorCLI crash when update drive firmware
SCGCQ00467119 - (Resolved) - SWR_SLES_11_SP3_GM Release validation : In storCli " serial number and FW package Build " fields are showing blank
SCGCQ00469179 - (Closed) - Aligning with FW for strip calculation for 4K drives
SCGCQ00372264 - (Closed) - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00374377 - (Closed) - GetGGEEPData equivalent syntax is not present in storcli
SCGCQ00374418 - (Closed) - Storcli : controller information query is displaying the status as failure.
SCGCQ00375757 - (Closed) - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
SCGCQ00377364 - (Closed) - StorCli shows Power Saving Option as enabled, despite controller having power saving option completely disabled.
SCGCQ00380889 - (Closed) - Not able to set securitykey on controller
SCGCQ00381100 - (Resolved) - MR: not able to create PRL11 using 96 drives.
SCGCQ00383043 - (Closed) - StorCLI-Invader : The "coercion" mode is not in sync with the legacy values.
SCGCQ00384644 - (Resolved) - iMR_Inv_6.1:StorCLI- StorCLI does not show 'Unsupported/Blocked' state for 4K drives even though FW is not supporting 4K
SCGCQ00386586 - (Closed) - include support for SWR controllers in non LSI verison of storcli.
SCGCQ00394127 - (Closed) - Added the command to DOS SCU
SCGCQ00394883 - (Closed) - StorCli_MR: While Creating RAID1 with four drives command facing the "C0:BAIL_OUT at line 1354"
SCGCQ00396303 - (Resolved) - Cfgclr command fails without force option in Sparc OS
SCGCQ00400019 - (Closed) - "storcli /c0/dall show" command not working
SCGCQ00411501 - (Closed) - StorCli_MR: Cache vault Strart learn command displaying twice in the hep file "/c0/cv h"
SCGCQ00414328 - (Closed) - Perf mode value not getting set when executed along with the other parameters
SCGCQ00414731 - (Closed) - Checking in StorcliF & storcli0 changes
SCGCQ00415454 - (Closed) - StorCLI help file does not display "add vd spanned array"
SCGCQ00420040 - (Closed) - StorCLIF : Not able to read or write factory settings with adpsettings command (legacy command )
SCGCQ00436928 - (Closed) - Illusive/Bad Data Extracted
SCGCQ00437762 - (Closed) - Exit code coming as 1 for adpbios (Megacli Syntax)
SCGCQ00443072 - (Closed) - SWR: In Store Cli if we start any background operation Estimated time left field showing Blank
SCGCQ00447686 - (Closed) - Storecli does not display complete information for the command ./storecli /c0/p0-x show.
SCGCQ00456501 - (Closed) - StorcliF: StorcliF and StorcliO crashes when given invalid file for the command /c0 set factorysettings file=filename
SCGCQ00460861 - (Closed) - MR_Inv_6.1:StorCLI- Gives wrong message after battery retention test command is issued for Supercap FBU03
SCGCQ00466038 - (Closed) - MR_Inv_6.1:StoreCLI- StorCLI reports retention time as 0 for supercap FBU02 and FBU03
SCGCQ00469162 - (Closed) - In virtual drives information the Cac filed values are incorrect with regular VD's
SCGCQ00379157 - (Closed) - StorCLI: the help file for "storcli /cx transform iMR" is missing
SCGCQ00380143 - (Closed) - The set phy linkspeed operation needs to have the unit(GB/s) mentioned and the Description" column is blank for set and Show.
SCGCQ00394952 - (Closed) - Segmentation fault hitting while executing the command "/c0 set bgi h "
SCGCQ00398246 - (Closed) - VD create syntax display improper output.
SCGCQ00398992 - (Closed) - Command displayed in the same line after "Press any key to continue".
SCGCQ00402499 - (Closed) - Storecli /c0 show eventloginfo 
SCGCQ00403335 - (Closed) - Mismatch of "Start Copyback " command in global help file and particular help file of copyback .
SCGCQ00436538 - (Closed) - pd version is not listing all if PDs are missing
SCGCQ00442610 - (Closed) - Onfi_patch_6.0:Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00447972 - (Closed) - Storcli : adpgetprop command for enableeug/enableeghsp showing success and not getting reflected when we give wrong flag
SCGCQ00451393 - (Closed) - Megascu adpm0flash command hangs
SCGCQ00462885 - (Closed) - Need to remove storcli /cx show clusterenable and storcli /cx set clusterenable=<value> since FW did not support this in HA
SCGCQ00364097 - (Resolved) - iMR_Inv_6.1:StoreCLI- StoreCLI reports wrong Emulation type for VDs
SCGCQ00375625 - (Closed) - StorCLI : Displaying failure in the output for querying Dimmer switch information
SCGCQ00379104 - (Closed) - Not able to get paged view of StorCLI output on VM-Ware Platform
SCGCQ00390777 - (Closed) - iMR_Inv_6.1:StorCLI- VD creation command does not give any message if we tried to create a PI VD using normal PDs
SCGCQ00392598 - (Closed) - Pause operation should be sync with in show status of the PR.
SCGCQ00392686 - (Closed) - For the perfmode command in the help file we are displaying the storcli.exe /cx set perfmode = <value> syntax
SCGCQ00393442 - (Closed) - Spelling mistake in keyword headlessSafeMode
SCGCQ00406580 - (Closed) - Adprestart command fails
SCGCQ00413803 - (Closed) - Factory Command /c0/bbu start retentiontest should not be supported in storcli
SCGCQ00438350 - (Closed) - Megacli crashes after invoking any command in system with one 9280-8e and 2 quad port qlogic FC cards.
SCGCQ00457906 - (Closed) - storcli_6.1:The help file for"./storcli /cx/mx set h " is missing
SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00380746 - (Closed) - Error handling for Drive FW download when the hardware is not supported.
SCGCQ00384729 - (Closed) - Storcli-Inv-multiple VD's in same DG, setting security using /cx/vall set security=on is Failing for every VD except 1st VD
SCGCQ00392501 - (Closed) - StorCli_5.7 : "/c0/bbu start learn h " is not showing.
SCGCQ00394005 - (Closed) - Enabling OCR from StorCLI actually disables the controller property.
SCGCQ00394375 - (Closed) - Adprestart command fails
SCGCQ00397920 - (Closed) - StorCli_MR: BBU Strart learn command displaying twice in the "/c0/bbu h"
SCGCQ00400025 - (Closed) - Storcli shows inaccurate Elapsed Time as recon progresses
SCGCQ00400640 - (Closed) - Copyright information is showing wrongly
SCGCQ00408070 - (Closed) - StorCLI does not show both "Current Write Policy" and "Default Write Policy" for VD
SCGCQ00423347 - (Closed) - Storclif :Segmentation Fault with execution of legacy command BBUMFGSET .
SCGCQ00423832 - (Closed) - EFI_ Storcli: Cannot set vpd file on controller, EFI hangs and cannot proceed for further operations until reboot
SCGCQ00433513 - (Closed) - StorcliF : Not able to get or set connector mode on cassiopeia controller
SCGCQ00436931 - (Closed) - CLI displays VPD data for TMM and Battery/Supercap = ONLY TMM Data Extracted but NOT Supercap Data
SCGCQ00449134 - (Closed) - Battery Over-temp is not showing correctly.
SCGCQ00454427 - (Closed) - Storcli_6.1:"press any key to continue" showing twice in the lagacy command
SCGCQ00464708 - (Closed) - Storcli display total number of VDs in a individual drive group properties.
SCGCQ00369258 - (Closed) - Description is shown as "None" when using verchk option while flashing fw.
SCGCQ00392053 - (Closed) - MegaCLI and StorCLI should display "Estimated Time Left" in hours, days and minutes format.
SCGCQ00396665 - (Closed) - StorcLi_5.7: Remove the description for "Ra=Read Ahead Adaptive" in VD show info.
SCGCQ00397663 - (Closed) - StorCli_MR: While creating VD using default values FW allows read policy as"Ra=Read Ahead Adaptive" as against PR-317400
SCGCQ00399443 - (Closed) - StorCLI App Crash while execution of event info for vd ccincon
SCGCQ00402910 - (Closed) - StorCli_6.0:Raid level can be created even wthout delimiter(i.e size=1gb1gb1gb1gb)
SCGCQ00424978 - (Closed) - Is VD Emulated=Yes when emulationType=1
SCGCQ00436107 - (Closed) - The bootwithpinnedcache logic is backwards, both storcli and the FW are affected
SCGCQ00448094 - (Closed) - core dump while issuing storcli command ./storcli /c0/fall show all.
SCGCQ00454971 - (Closed) - storcli /c0 show is not listinf SWR controller
SCGCQ00378448 - (Closed) - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
SCGCQ00395178 - (Closed) - storcli doesnt support legacy MegaCli elf commands
SCGCQ00400139 - (Closed) - StorCLI shows date of manufacture in non-convention format
SCGCQ00413789 - (Closed) - storcli crashes on having a non PI drive and trying to create pi vd on all the drive
SCGCQ00422006 - (Closed) - Storcli crashes when given wrong in put file to set VPD on controller
SCGCQ00442444 - (Closed) - MR_Inv_6.1:StoreCLI- StorCLI gives wrong info when preserved cache is generated on 4K VD (./storcli /c0 show preservedcache).
SCGCQ00442652 - (Closed) - SWR_1.34 - Serial number field is blank in controller information and the same could be updated with N/A in StorCli
SCGCQ00066241 - (Closed) - MPI 2.5: Power Management
SCGCQ00308453 - (Closed) - MPI2: IR reporting Elapsed Seconds
SCGCQ00299943 - (Closed) - MPI2: add IOCExceptions bit for Partial Memory Failure
SCGCQ00250721 - (Closed) - MPI2: Update Hard Reset Algorithm with new timings
SCGCQ00209048 - (Closed) - MPI2: Return Port info in the SAS Device Status Change Event
SCGCQ00201727 - (Closed) - MPI2: Add spin-up disable bit to SAS IO Unit Page 4
SCGCQ00201203 - (Closed) - MPI2: Remove/Obsolete MPI Power Management Control Feature PCIE_LINK
SCGCQ00194293 - (Closed) - MPI2: product specific range for extended image type
SCGCQ00116336 - (Closed) - Gen 3: method to enable/disable FastPath capability on a per-device basis
SCGCQ00125672 - (Closed) - Gen 3: add 12Gb/s option for link rate
SCGCQ00125683 - (Closed) - MPI2: add Link Rate of UNSUPPORTED_PHY_ATTACHED
SCGCQ00136677 - (Closed) - Gen3: add optional vendor-unique region to MPI25_SCSI_IO_REQUEST structure
SCGCQ00137514 - (Closed) - MPI2: add PCI Device ID for Warhawk
SCGCQ00138259 - (Closed) - MPI2: add alternative defines for SGE Direction bit
SCGCQ00140397 - (Closed) - MPI2: modify Host Based Discovery Action Request
SCGCQ00141834 - (Closed) - MPI2: ability to disable SATA NCQ on a per-device basis
SCGCQ00155192 - (Closed) - MPI 2.5: update PCI Device Ids for Invader / Fury
SCGCQ00157968 - (Closed) - MPI2: Add new Config Page Type - Extended Manufacturing
SCGCQ00159010 - (Closed) - MPI2: MFG 7 update: method to link ISTWI devices, GPIO, PHYs of a SAS connector
SCGCQ00160485 - (Closed) - MPI2: Change MPI Simple SGE Local bit description and IEEE Chain Flags to match HW
SCGCQ00161661 - (Closed) - MPI2: Add IOC Temperature Monitoring Capability
SCGCQ00162562 - (Closed) - MPI2: rework Pinout field of ConnectorInfo for MFG Page 7
SCGCQ00162597 - (Closed) - MPI2: reserve some FWDownload ImageType values for product-specific use
SCGCQ00163413 - (Closed) - MPI2: IOUnit page 7: Add new fields for Board temperature
SCGCQ00163641 - (Closed) - MPI 2.5: SCSI Initiator I/O path counters (SAS IO Unit Page 16)
SCGCQ00164407 - (Closed) - MPI 2.5: review SGE Flags for Local bit and Data Location Address Space changes
SCGCQ00166171 - (Closed) - MPI2: new event for NOTIFY(Enable Spinup)
SCGCQ00176893 - (Closed) - MPI 2.5: new Power Performance Change Event to report changes to global power management mode
SCGCQ00177635 - (Closed) - MPI 2.5: report offset of first EEDP error in SCSI IO Reply
SCGCQ00268818 - (Closed) - Allow for MPI 2.5 IEEE Chain Element in SATA Passthrough Request
SCGCQ00283196 - (Closed) - Toolbox Diagnostic CLI Request now uses IEEE SGL, including chain elements
SCGCQ00378774 - (Implemented) - new storcli object is added to storcli to represent cachevault
SCGCQ00413314 - (Implemented) - Implement storclif commands - get/set hwdevice and configpage
SCGCQ00413317 - (Implemented) - Implementation of StorCLIF command for AdpSetSubOEMId XX -aN and AdpGetSubOEMId -aN
SCGCQ00421090 - (Closed) - Added the HA code to MR5.8 stream
SCGCQ00425077 - (Implemented) - Set factory default command in StorCLI
SCGCQ00283198 - (Closed) - MPI2: Toolbox Diagnostic CLI Tool Request may now use chain elements in the SGL
SCGCQ00258327 - (Closed) - MPI2: Reserve Product Specific range for Event codes
SCGCQ00229719 - (Closed) - MPI2: BIOS Page 1 additions for UEFI HII
SCGCQ00228572 - (Closed) - MPI2: add 4K sectors supported bit to IOC Page 6 CapabilitiesFlags field
SCGCQ00203886 - (Closed) - MPI2: New RAID Action (COMPATIBILITY_CHECK)
SCGCQ00194461 - (Closed) - MPI2: Add auto reserve and 8-kbit seeprom support to ISTWII
SCGCQ00128142 - (Closed) - Gen 3: update MPI v2.5 header files
SCGCQ00132183 - (Closed) - MPI2: add optional vendor-unique region to MPI2_SCSI_IO_REQUEST structure
SCGCQ00136201 - (Closed) - MPI2 - additional IR status information
SCGCQ00142578 - (Closed) - MPI2: obsolete MPI2_IOUNITPAGE1_MULTI_PATHING
SCGCQ00169936 - (Closed) - MPI 2.5: remove Command Determines Data Direction bit from SCSI IO
SCGCQ00172984 - (Closed) - MPI2: for SRIOV, allow PF to access config pages for other VFs
SCGCQ00175997 - (Closed) - MPI2: Add IO Unit Page 10 - Host Credit Balancing
SCGCQ00218764 - (Closed) - MPI2: new name for SCSI IO Request Control bits
SCGCQ00227491 - (Closed) - MPI 2.5: IR - new Raid Action to enable the Fast Path
SCGCQ00209055 - (Closed) - MPI2: create product-specific range for RAID Action Request
SCGCQ00125496 - (Closed) - Gen 3: remove Release On Full option for diag trace buffer
SCGCQ00159395 - (Closed) - MPI 2.5: Obsolete MPI2_RAID_VOL_CREATION_BACKGROUND_INIT
SCGCQ00175743 - (Closed) - MPI2: method to communicate between hosts on virtual functions
SCGCQ00433477 - (Implemented) - Mapping of MegaCLI(DPMenable(set/get) & ForceSGPIO(get/set) command to StorCLI( (show/set -> DPM) & (show/set SGPIOforce))
SCGCQ00438735 - (Closed) - Changed the storcli syntaxes as Suggested by PDM's and FAE's.
SCGCQ00157982 - (Closed) - MPI 2.5: Chain SGL Segment sizes
SCGCQ00399602 - (Implemented) - storcli support for LSI and OEM, factory
SCGCQ00412981 - (Implemented) - implementation of StorcliF commands for adpsetsasa,adpdiag,adpshutdown
SCGCQ00435665 - (Implemented) - storcli mapping for the missing legacy commands
SCGCQ00125662 - (Closed) - MPI2: review Task Set Full handling
SCGCQ00353002 - (Implemented) - Signed FW Update
SCGCQ00375811 - (Closed) - Need MegaSCU for changes in MFC
SCGCQ00380155 - (Implemented) - Undo - blocking firmware update for drives behind ALTA
SCGCQ00413337 - (Implemented) - MWCLI. storcli builds for LSI and OEM factory, please check description.
SCGCQ00137489 - (Closed) - MPI2: bring Diagnostic Data Upload Tool forward from MPI v1.5
SCGCQ00379169 - (Implemented) - Remove support for flashing firmware on PDs behind ALTA
SCGCQ00413064 - (Implemented) - Implementation of MegaSCU commands in storcli syntax
SCGCQ00413432 - (Closed) - Implementation of commands mentioned in the desc below
SCGCQ00441143 - (Implemented) - Implementing Bad block management related comands in storcli.
SCGCQ00369601 - (Implemented) - MWCLI. Add -adpbattest capability to EFI CLI
SCGCQ00369604 - (Implemented) - Rebuild time reset
SCGCQ00381311 - (Implemented) - dcmd path chagnes for supporting the new cachevault api
SCGCQ00419161 - (Implemented) - Implementation of StorCLIO command for ADPMFGSET -f file a0 in storcli
SCGCQ00419336 - (Implemented) - Implementation of setPcilinkspeed command in storCLIF
SCGCQ00423256 - (Closed) - RRB 45 - CLI Reporting of TMM VPD
SCGCQ00369742 - (Implemented) - MWCLI. R10, R50, R60, R00 VD creation
SCGCQ00381093 - (Implemented) - PR SCGCQ00319011: Rebuild time reset
SCGCQ00433703 - (Implemented) - Megacli/storcli support for lmrc driver
SCGCQ00434744 - (Implemented) - Equivalent storcli command implementation of MegaCLI -AdpGetPciInfo -aN|-a0,1,2|-aALL
SCGCQ00447069 - (Implemented) - Implementation of StorCLIO command for Adpnvram clear a0 in storclio as well as support legacy command
SCGCQ00413330 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00413856 - (Port_Complete) - remove the "Drive write cache" policy from Pd information.
SCGCQ00417917 - (Port_Complete) - UEFI StorCli doesn't show the correct UEFI Driver Version
SCGCQ00413017 - (Port_Complete) - Storcli reports "segmentation fault" when running command to downgrade controller to iMR
SCGCQ00413888 - (Port_Complete) - StorCli_6.0-The help file for "storcli /cx/dx set security " is missing
SCGCQ00376240 - (Port_Complete) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00411384 - (Port_Complete) - Unable to start migration from R0 to R5
SCGCQ00411614 - (Port_Complete) - hits segmentation fault while creating multiple Vd's on Raid 10.
SCGCQ00413311 - (Port_Complete) - Cannot change or update controller date and time in MegaSCU
SCGCQ00437065 - (Port_Complete) - Driver Version is not shown
SCGCQ00375839 - (Active) - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00411449 - (Port_Complete) - Improper output when configure R10 VD.
SCGCQ00414863 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00413041 - (Port_Complete) - Getting error message while installing or upgrading on Linux platform
SCGCQ00458499 - (Port_Complete) - Block configuration with unsupported strip element sizes
SCGCQ00414383 - (Port_Complete) - When a command fails, subsequent commands/actions are aborted in storcli (MegaCli)
SCGCQ00391744 - (Active) - StorCli-"show ctrlcount" help is not displaying.
SCGCQ00412593 - (Port_Complete) - Resolving compiler errors for Ctrl-R
SCGCQ00425263 - (Active) - storcli /c0 show all : did not have HA information+request to add additional info


Installation Commands: 
=======================
Refer to the User's Guide included in the package.





Component:
=========
SAS MegaRAID StorCLI
Release Date: 05/30/13


Version Numbers:	StorCLI
===============		===========			
Current Version		1.04.07
Previous Versoin	1.03.11


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris
FreeBSD
EFI 
Ubuntu

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00364332 - (Closed) - StoreCLI does not give proper message while trying to create 33rd VD on iMR FURY controller
SCGCQ00374336 - (Closed) - System halts on issuing storcli commands in EFI Environment.
SCGCQ00374732 - (Closed) - StorCLI cannot set "bypasserror" or "be"
SCGCQ00374733 - (Closed) - Storcli does not show 512 strip size in the online help
SCGCQ00378124 - (Closed) - Porting of AdpRestart Command
SCGCQ00372155 - (Closed) - Certain controller features displayed under "show all" exceeds 80-char limit.
SCGCQ00374118 - (Closed) - StorCli-"/c0/dall show all "in FreeSpaceDetails legend missing for "ID/VD/AfterVD"
SCGCQ00378135 - (Closed) - portings of AdpRestart command
SCGCQ00378828 - (Closed) - StorCLI-Legacy:'adpbootdrive get' fails to get bootdrive information.
SCGCQ00372264 - (Closed) - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.
SCGCQ00374418 - (Closed) - Storcli : controller information query for OEM controller is displaying the status as failure.
SCGCQ00375757 - (Closed) - "StorCLI /cx/bbu show modes" show the bbu modes description without the actual bbu mode number
SCGCQ00374735 - (Closed) - StorCLI crashed when run on a Windows 2008 64-bit with 24GB of RAM and 66 drives attached
SCGCQ00380746 - (Closed) - Error handling for Drive FW download when the hardware is not supported.
SCGCQ00369258 - (Closed) - Description is shown as "None" when using verchk option while flashing fw.
SCGCQ00378448 - (Closed) - StorCLI reports incorrect message when download a firmware image to the controller with pinned cache
SCGCQ00375811 - (Implemented) - Need MegaSCU for changes in MFC
SCGCQ00380155 - (Implemented) - Undo - blocking firmware update for drives behind interposer
SCGCQ00379169 - (Implemented) - Remove support for flashing firmware on PDs behind interposer
SCGCQ00375839 - (Active) - StorCLI: The legend for "phy Error Counters" exceeds the 80-char limit.

Installation Commands: 
=======================
Refer to the User's Guide included in the package.





Component:
=========
SAS MegaRAID StorCLI
Release Date: 03/02/13


Version Numbers:	StorCLI
===============		===========			
Current Version		1.03.11
Previous Versoin	1.02.08


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris
FreeBSD
EFI 

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
SCGCQ00339670 - (Completed) - Fixing Linux Release 1.02-00
SCGCQ00359141 - (Completed) - Fixing Linux Release 1.03.01


Installation Commands: 
=======================
Refer to the User's Guide included in the package.






Component:
=========
SAS MegaRAID StorCLI
Release Date: 01/16/13


Version Numbers:	StorCLI
===============		===========			
Current Version		1.02.08 (Phase 3)
Previous Version	1.01.10 (Phase 2)


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN
Solaris
FreeBSD
EFI (EFI StorCLI version 2.5.1.02.05)

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
There were few updates in command syntaxes. 
-	See revision history in Rev E : available in Page 2 of user guide(StorCLI_Phase3_RefMan_.pdf)
-	See revision history in appendix D: available in Page 76 of user guide(StorCLI_Phase3_RefMan_.pdf)
SCGCQ00295690	MWCLI. Solaris x86 support
SCGCQ00295810	MWCLI for uEFI
SCGCQ00314895	MWCLI. FreeBSD 7.x & 8.x support
Fixes since Phase 2 Release...
SCGCQ00374892	XD1.5-StorCLI attempts to Add/remove configure/unconfigured VDs when add/removal of ALL vds is issued.
SCGCQ00355952	StorCLI : Not able to set CC scheduling beyond some limit.
SCGCQ00356883	Storcli - legacy commands related to bbu failing in multicontroller environment
SCGCQ00345353	storcli /c0/ex show status---> It is not displaying all the information of the enclosure.
SCGCQ00356970	StorCLI: The time remaining column is not populated on executing "storcli /c0 show aso" and no description for "Mode" column.
SCGCQ00358752	StorCLI: "/c0 show" command displays PD LIST table information occupying more than 80 coloumns
SCGCQ00360027	StorCli-Incorrect VD size displayed after expansion of VD size.
SCGCQ00335385	Storcli command won't display any controllers
SCGCQ00339764	StorCLI_EFI : Getting syntax error for add hotsparedrive command.
SCGCQ00343802	StorCLI_EFI : System halts on performing  RLM (Raid level Migration)  without adding/removing drives, in EFI Environment
SCGCQ00352972	StorCli- system halted on executing command " storcli /c0/f show"  in UEFI
SCGCQ00354167	StorCli- "System hang" while creating the VD using legacy command in UEFI
SCGCQ00354581	Storcli_EFI : System halts while executing lengthy commands
SCGCQ00315799	4k_DIF: Not able to Replace the missing Drive for 4K VDusing the MegaCLI -Vogel_1.0_sprint_4k Apr 11, 2012
SCGCQ00315801	Creating the 4K VD fails with firmware error description using MegaCLI -Vogel_1.0_sprint_4k
SCGCQ00316591	Storcli: Importing Foreign Configuration while Rebuild is in progress Show fall shown multiple R60 VDs
SCGCQ00316673	Storcli: Query for Phyinfo using storecli twice, will results in non-functional controller/system hang
SCGCQ00316674	Unable to set abortCConerror property on controller card using StoreCli.
SCGCQ00316675	Storcli displaying Emergency spare is No for all unconfigured drives while "enableeug" property is ON
SCGCQ00337971	StorCLI : Not able to schedule PR in EFI environment
SCGCQ00338386	StorCLI : Not able to upgrade controller firmware  without using nosigchk and noverchk in EFI Environment.
SCGCQ00338398	StorCLI: getting syntax error for pd insert command in EFI Environment
SCGCQ00341481	StorCLI - after migration the last pd is getting displayed twice( when migrating from 4pd raid 5 to 6 pd r0 )
SCGCQ00341581	Set path to new library as "export LD_LIBRARY_PATH=/usr/local/lib" after installing libgcc-3.4.6-sol10-x86-local.pkg
SCGCQ00341585	fails to log the latest set of events to the file.
SCGCQ00341991	StorCLI_EFI: Displaying "" symbol under progress bar when PD Initialization is in progress
SCGCQ00342017	StorCLI: After a controller FW flash from StorCLI, No pending Images are seen before a reboot as seen in the legacy builds.
SCGCQ00342072	FreeBSD - Adapter cache Flush is not working .
SCGCQ00342077	storecli_EFI.storecli.efi /c0/pall set linkspeed=val   It is not displaying PHY info field .
SCGCQ00342117	StorCli does not display a help message for  "/cx/ex show status h" and storCLI  storcli /cx/ex show all h
SCGCQ00342241	StorCLI_EFI:Storcli is showing that VD expansion is possible but not allowing to expand if space is before start LBA of VD
SCGCQ00342272	StorCLI_EFI : Not able to save the configuration with Megacli syntax
SCGCQ00342670	StorCli-"enblPI/PreventPIImport" equivalent command is not their in StorCLi
SCGCQ00342693	StorCLI: A Drive spinup/spindown not successful on drives marked as hotspare as against MSM.
SCGCQ00342730	Storcli_EFI : Not getting valid JSON output for any of the commands in EFI Environment
SCGCQ00342732	StorCLI: the "set bootdrive = on" command sets the requested vd2 as bootable without user intervention.
SCGCQ00343591	StorCLI: A dedicated hot spare cannot be assigned to any one of the particular spans for a spanned DG as against MSM.
SCGCQ00343636	StorCLI allows a single Unconfigured Drive to be assigned as a dedicated hotspare to two different VD's.
SCGCQ00343799	StorCLI: Cannot explicitly assign the configured cachecade VDs to the Disk Groups for the existing CC-VD.
SCGCQ00345525	StorCLI: On performing an "add vd" with size provided in TB a decimal value is truncated to whole number as input.
SCGCQ00345557	StorCLI:  A vd can be assigned to a cachecade VD multiple times also a cachecade VD allows to be assigned to itself.
SCGCQ00345791	Storcli: not able to flash PD firmware on FreeBSD
SCGCQ00346878	Storcli: Not getting proper import preview for secured foreign VD on EFI and Solaris Environment.
SCGCQ00346917	Storcli_EFI : Not able to set securitykey on controller in EFI environment
SCGCQ00348494	StorCli-" /c0 show stoponerror" is not working
SCGCQ00350582	StorCli- "Disk Group" column is missing.
SCGCQ00353580	Storcli- "/c0/fall show" is displaying wrong.
SCGCQ00353641	StorCLI - spinup/spindown is not supported for tape drive , but executing spindown operation shows success message
SCGCQ00356700	StorCLI - legacy command adpshutdown not working properly
SCGCQ00356986	StorCLI - when " stop initialization " command is executed on a pd even when it is not in progress it is showing success
SCGCQ00357024	StorCLI - flush|flushcache showing command not supported whereas subsequent legacy command working successfully
SCGCQ00360565	In '/cx/vx show all' Active Operations = None during a Rebuild
SCGCQ00289586	Emulated Block size should be displayed as part of PD information for 512E drives
SCGCQ00316676	StorCLI help does not have the information to show the boot drive
SCGCQ00316680	FreeBSD support for MegaWare Cli
SCGCQ00318116	StorCLI2.5: "delay" & properties of "Consistency Check" does not function properly
SCGCQ00320538	iMR_Inv_MegaCli:Deb package fir MegaCli not available for Ubuntu 12.04 OS
SCGCQ00324813	MegaCLI: MFI_STAT_NOT_FOUND returns when retrieving the FW event log.
SCGCQ00326760	StorCli adpbbucmd shows next learn cycle would happen 1 day earlier for SuperCaP
SCGCQ00327419	StorCli-IN help file-"BBU show status" command is not their.
SCGCQ00327557	Storcli-"BBU show help" is not working.
SCGCQ00328182	StorCLI2.0: patrolread help description for delay is mentioned in terms of "minutes" instead of "hours"
SCGCQ00328204	StorCLI- Individual help for VD expansion does not give the completion description .
SCGCQ00328568	StorCli-"PHY Linkspeed show help/" is not working
SCGCQ00329941	StorCli-"DRIVER VERSION" is not displaying for SWR controller  on LINUX Platform.
SCGCQ00330263	StorCli-" show  ds | safeid | rehostinfo help" is not displaying.
SCGCQ00330447	StorCli-" On VD show cc help " is not displaying
SCGCQ00335327	storcli 1.01.10 doesn't display all required enclosure info for /cx/ex show all, i.e. voltage/ps/temp/etc status/values
SCGCQ00337951	Storcli : Exit code is displayed  unnecessarily at the end of output on efi environment .
SCGCQ00337956	StorCLI: -h is not working for help display in  efi environment
SCGCQ00337967	StorCLI : getting invalid error code (out of range) while querying for invalid drive number in EFI Environment
SCGCQ00338155	StorCLI : VD's exluded from CC Scheduling is not reflected properly with /c0 show cc command in EFI Environment
SCGCQ00338194	StorCli-IN help file-"BBU show properties" command is not their.
SCGCQ00338206	StorCli- "legacy help file is not displaying"
SCGCQ00338265	StorCLI: paged view of any output should support " Press any key to continue" to proceed to next page
SCGCQ00338393	StorCLI : Date and Time of controller is not displayed in proper format in EFI Environment
SCGCQ00338576	StorCli-"Help page" last line execuite with storcli directory.
SCGCQ00339730	StorCLI_EFI : In paged output the lines following the message "Press any key to continue" should be displayed in next line.
SCGCQ00340208	code changes for some StorcliEFI-DEFECT
SCGCQ00341443	StorCLI - partial help for patrolread delay is not working
SCGCQ00341451	StorCLI - show patrolread is not showing the progress of the current patrol read in percentage
SCGCQ00341472	StorCLI - show migrate is not displaying the time since the virtual drive migration started
SCGCQ00341679	StorCLI : partial help for cc is not working ("/cx show cc h" ) . Giving syntax error
SCGCQ00342053	storecli_EFI>storecli h  It is displaying description of some commands(use only for partial help).
SCGCQ00342122	help file is not available for  "storcli dx show all h"
SCGCQ00342129	storecli_EFI> storecli.efi /c0/ex show status not displaying ALARM info field
SCGCQ00342144	StorCLI - the command "./storcli /c0 show reconrate " is displaying the migrate rate under controller prop
SCGCQ00342229	storecli_EFI> After stopping init in multiple vds ,VD status in not updating properly.
SCGCQ00342461	StorCLI doesn't show NCQ support of a SATA drive
SCGCQ00342597	StorCli-"Perfmode" value is not mentioned in the description
SCGCQ00342605	StorCLI does not prompt user intervention while deleting VD which has Boot Partition.
SCGCQ00342727	Help description for Controller Properties abbrevations like ABS, SOE is missing in cmd O/P
SCGCQ00342737	Not displaying the correct version of driver in megacli command.
SCGCQ00342997	StorCLI - not getting partial help for /cx/px set linkspeed h
SCGCQ00343108	StorCLI_EFI : Not able to disable/enable  Dimmer switch 1 with command /c2 set ds=off/on  type=4
SCGCQ00343191	StorCLI - cannot get a helpfile for "./storcli /cx set cc h "
SCGCQ00343199	StorCli-In Help File" show/set OCR" command is not their.
SCGCQ00343222	FREE BSD- Modifiaction of syntax required in help file for setting consistency check .
SCGCQ00343682	StorCLI - Syntax of set cc is given wrong in global help file
SCGCQ00343749	StorCLI: mismatch with help file for setting linkspeed with the that of the error message on setting unsupported linkspeed.
SCGCQ00343786	StorCLI -  "storcli /cx delete securitykey"when executed twice in a row shows a success status in controller properties
SCGCQ00344142	The size is in KB for "WithArrExp" instead of GB under EXPANSION INFORMATION
SCGCQ00344188	Help file not working for 'storcli /cx/vx expand '
SCGCQ00344707	StorCLI: 512KB Stripe size is not mentioned in CLI  help page of "storcli /cx add vd h"
SCGCQ00345311	StorCLI - "storcli /cx/pall set linkspeed = 1.5/3 ... " showing success but setting it individual is showing a comand invalid
SCGCQ00345706	./storcli /c0 set perfmode=val  ----->It is setting perfmode value other than 0 and 1
SCGCQ00345907	StorCli-" show aso " command is missing in help file.
SCGCQ00346025	./Storcli -AdpGetPciInfo -a0 ---->This command is not displaying information like bus,device,functional no. of the adapter.
SCGCQ00346919	Storcli_EFI : partial query for commands is not working with numbers like /c0 set h (works only with /cx )
SCGCQ00348538	StorCli-"Firmware Package Build" version is not showing in controller Info (UEFI)
SCGCQ00348706	StorCli-"/c0 set ds h" in help description need to some changes.
SCGCQ00349475	StorCLI: The "gas gauge" needs to be addressed under "show BBU status h"
SCGCQ00349498	StorCLI: A help file to be added for "storcli /c0/bbu start learn"
SCGCQ00351169	./storcli /c0 set securitykey=xxx passphrase=xxx ---->Description of securitykey should be display in description field.
SCGCQ00351987	Storcli : Unexpected line at output when legacy command ''Adpallinfo'' executed with page=x
SCGCQ00352560	The help file for "set backplane" needs to be revised.
SCGCQ00352571	StorCLI: "The set backplane = 0"  the command value description exceeds 80 charecters.
SCGCQ00352630	STORCLI: Command to set SOE(stop on Error) is missing in global help file
SCGCQ00352637	StorCLI: Global/Individual help missing for command to set ABS(Auto Boot Select) .
SCGCQ00352779	User guide PDF file for Technical and Documentation are required to be updated.
SCGCQ00352887	None of the build is having readme file except solaris in the storcli build ---->ver 1.02-02 Oct 23,2012
SCGCQ00353682	Storcli- Displaying incomplete foreign config even if all the drives are in Ugood state for /c0/fall show command
SCGCQ00353683	after controller firmware download completes Description is showing the firmware package version instead of firmware version
SCGCQ00354235	Storcli: StorCLI  should throw syntax error for the command /c0/dall show all all all
SCGCQ00354543	StorCLI: help legend missing for "show freespace"
SCGCQ00355107	StorCLI-Require Update of the URL mentioned in Readme File of SOLARIS11 .
SCGCQ00355116	Storcli_EFI : Showing success for  non-supported operations,  related with  association of VD to cachepool.
SCGCQ00355137	Storcli - when setting smartpollinterval to -1 , it is throwing syntax error instead of failure .
SCGCQ00355367	StorCLI- Description for what kind & range of value will be accepted by memscrubpatterns is not provided in help file
SCGCQ00355432	StorCLI : Not able to set CC execution delay if used with complete  CC scheduling command
SCGCQ00356657	Special Charecters are printed or the state info is missing under the state column of the drive.
SCGCQ00356695	StorCLI - when stop command for PD reated operations  is executed . The command description shows wrong slot id's for PD's
SCGCQ00356998	Storcli-display command when used with "page" is not showing the output correctly...
SCGCQ00357319	The "EID:Slot" is not populated on fetching information on the existing foreign configuration.
SCGCQ00357371	StorCLI: The PD list table is not sorted acoording to enclosureid:slotid.
SCGCQ00357647	storcli: cliefimain.cpp file changes for lengthy commands.
SCGCQ00357648	Storcli reports baterry is charging and discharging at the same time.
SCGCQ00359371	Storcli-"show" info need to add  abbreviation for "PDs/DGs/VDs/BBU/Y"
SCGCQ00361544	StorCli-"/c0 start pr " in failure state displaying worng 'error message'.
SCGCQ00364859	Correcting the formats of below commands (exit code ,show event log and time, date format )
SCGCQ00328185	StorCli-In legacy help file command line execute  along with" press any key to continue"-only Windows OS
SCGCQ00328531	StorCLI2.0: phy linkspeed help description is mentioned in terms of "GB" instead of "Gb/s"
SCGCQ00333006	LSI MegaCLI EncInfo (Enclosure Info) duplicates the first power supply status data to both power supplies
SCGCQ00338675	'VD ADD' should use 'strip' instead of 'stripe'.
SCGCQ00341595	StorCLI - Spelling mismatch "Alta" specified which should either be "SATA" or "ATA"
SCGCQ00342071	storcli help command with "Legacy" and "page" option doesnt display the paged help.
SCGCQ00342978	StorCli-"Phy linkspeed show all help" in description spelling mistake is their.
SCGCQ00343142	StorCli-"eccbucketleakrate" , the value should be greater than ‘0’ and less than ‘65535’. Help is misleading.
SCGCQ00344136	Description for option [expandarray] in command storcli /cx/v(x|all) expand Size=<xx> is not clear
SCGCQ00344150	StorCLI - partial help ( Descripton ) for command "storcli /cx /bbu show properties h " is not there
SCGCQ00344171	StorCli-"Smartpollinterval"value need to be mention in the Description.
SCGCQ00344800	Help legend is missing for properties of enclosure in O/P of ./storcli /c0/e59 show all and show cmds
SCGCQ00344994	StorCLI - "storcli /cx/vx show preservedcache " command is not present in the help file
SCGCQ00352071	Storcli_EFI : "storcli -h legacy" cmd is not working
SCGCQ00352881	Alignment text issue in the O/P of command "storcli.efi /c0 show eventlogInfo"
SCGCQ00359980	Code cleanup in Univ_viva_cli
SCGCQ00340241	StorCLI - " insert " command is not working
SCGCQ00338560	StorCLI : Driver version is not displayed correctly
SCGCQ00339757	StorCLI_EFI : Progress field for drive erase operation is displaying "' symbol if drive erase is in progress.
SCGCQ00342762	StorCli-"Driver Version" field is missing (Free BSD 7.3)
SCGCQ00343005	StorCLI: Stripe Size of the VD is shown incorrect after a PD missing operation is performed on the disk group.
SCGCQ00346251	storcli does not report ROC temperature in '/cX show all' in HW section
SCGCQ00354427	StorCli-"System halts" on performing operation "/c0 set aso key=    " in UEFI
SCGCQ00342052	StorCLI - command "./storcli show " is throwing a description message that command is not supported
SCGCQ00343169	StorCli-"Show/set OCR help" is not Displaying
SCGCQ00344861	storecli_EFI > storecli.efi /c0 set perfmode h---> In  perfmode help file it is not giving what values we can set.
SCGCQ00346944	Storcli: Inquiry data of the drives is missing from output of  /cx/ex/sx show all command on FreeBSD with TB controller
SCGCQ00354191	Storcli - giving syntax error when trying to get help using numbers , e.g "storcli_efi /c0 h "
SCGCQ00355847	StorCli- "Serial Number" of physical Drives is not getting displayed in FreeBSD
SCGCQ00341986	StorCLI: Does not prompt the user to restart/reboot the controller after a FW flash for it to take effect as seen in MSM.
SCGCQ00348048	StorCLI: StorCLI does not provide single command to perform a locate drive configured as part of a VD as against MSM.
SCGCQ00348474	.\storCLI64.exe /c1 add vd type=r1 drives=47:1,2 ----> command is giving syntax error if using "comma" for vd creation.
SCGCQ00350579	StorCLI: The VD name cannot contain spaces as allowed in MSM.
SCGCQ00358917	EFI Shell StorCLI: Rebuild starts and does not make any progress in EFI env
SCGCQ00375019	“StorCli64.exe /xd/wdall show” command reports that NytroXD license is absent even when the license is available
SCGCQ00318433	Porting of Vogel 1.0 PRs to storcli phase 2.5
SCGCQ00341607	Failing to display Driver Version  in FreeBSd
SCGCQ00343664	Storcli-"Enclosure Slot No is mis matching "(DE1600-SAS )






Important Notes:
==================
STORCLI PHASE 2.0 Specific Limitations:
1.	User can use both 'raid0' and 'r0' for mentioning the raid level. And user can find both the forms in the help command.
2.	When passing parameter,'set' for CC mode is mandatory. 
3.	The use of comma in between array no and row parameter in the syntax for making ‘pdreplacemissing’ should not be used.
4.	User would not be able to specify ROWs while creating ‘Dedicated Hot Spare’. Instead user needs to use ‘Drive Group ID’ as dgs=N
5.	In ‘Foreign Configuration show’, utility will display VD as ‘Foreign’ instead of showing the VD state.
6.	The success code and description is printed only after complete processing of the command. Success will not be printed unless the entire log is displayed to the output. Hence the success code and description is printed at the end of the log for this particular command.
7.	Any command syntax is still valid, if user uses “-” instead of “/”  for e.g. storcli.exe /c0-vall show.
8.	Show ‘Bus and PCI Slot type’ are not shown as part of the controller information.
9.	While creating a VD using non-Enc-ID Devices, user needs to provide inputs in the format ‘D:SlotID’ as syntax (for eg: Drives=D:1,2,3 where 1,2,3 are the slot ids of the non encID devices)
10.	Tape Drives will be listed only with /c0/sall show all command, /c0/sall show doesn’t list Tape drive but only display the direct attached drives if present or a blank table if none are connected.
11.	Importing Foreign Configuration while Rebuild is in progress then query for Show fall the output would display multiple R60 VDs.
12.	Date and Time of controller is not displayed in proper format in EFI Environment 
13.	JSON is not required in EFI
14.	The sector size of the drives are displayed in “KB” instead of bytes under the PD List table. This is just display error in tabular format but it is displayed correctly in drive details.
15.	The “Eid:slot” column while importing a foreign config is not populated. StorCLI: The VD name cannot contain spaces as allowed in MSM.
16.	Consistency Check cannot be scheduled beyond year-2037AD.
17.	Flashing 9260CV low-level controller firmware is supported only through DOS version of CLI (MegaCLI) and not through EFI version of StorCLI.  Flashing MegaRAID firmware does not have this issue.

Known Behavior:
1.	‘All VD initialization’ command when run through StorCLI utility, shows the error message as failed for cachecaded VD. This is a generic limitation.
2.	While reconstruction is in progress, start of CC/Init/BGI operations on same VD throws an inappropriate error message. This is a generic limitation.
3.	In controller show cc the field CC current state will change only when it meets the schedule CC parameters.
4.	All the unsupported commands for SWR controller if tried to execute may result in unknown behavior for example – system hang-up. For the list of unsupported commands refer to user guide Appendix C: Unsupported Commands in Embedded RAID.
5.	Output for controller information contains junk characters in VMware ESXi 4.1 update2.  
6.	FDE drives are displayed as secured drives on SWR- SCU controller.
7.	There is no check to see whether user has entered different properties or the same property multiple times in StorCLI command. Hence StorCLI  does not throw syntax error for the command “/c0/dall show all all all”. This issue is because of the implementation of accepting multiple properties in a single command line in some cases.


Installation Commands: 
=======================
Refer to the User's Guide included in the package.




Component:
=========
SAS MegaRAID StorCLI
Release Date: 11/06/12


Version Numbers:	StorCLI
===============		===========			
Current Version		1.01.10


Contents:
=========
This package contains StorCLI for the following OSes:
Windows
Linux
VMware
VMware MN

Use the StorCLI components from the folder that matches your OS.


Enhancements and Bug Fixes
==========================
Initial Release


Important Notes:
==================
1.  User can use both ‘raid0’ and ‘r0’ for mentioning the raid level. And user can find both the forms in the help command.
2.  When passing parameter ‘set' for CC mode is mandatory. 
3.  The use of comma in between array no and row parameter in the syntax for making ‘pdreplacemissing’ should not be used.
4.  User would not be able to specify ROWs while creating ‘Dedicated Hot Spare’. Instead user needs to use ‘Drive Group ID’ as dgs=N
5.  In ‘Foreign Configuration show’, utility will display VD as ‘Foreign’ instead of showing the VD state.
6.  The success code and description is printed only after complete processing of the command. Success will not be printed unless the entire log is displayed to the output. The success code and description is printed at the end of the log for this particular command.
7.  Any command syntax is still valid, if user uses “-” instead of “/”  (e.g. storcli.exe /c0-vall show.)
8.  Show ‘Bus and PCI Slot type’ are not shown as part of the controller information.
9.  While creating a VD using non-Enc-ID Devices, user needs to provide inputs in the format ‘D:SlotID’ as syntax (e.g. Drives=D:1,2,3 where 1,2,3 are the slot ids of the non encID devices.)
10. Tape Drives will be listed only with /c0/sall show all command. /c0/sall show doesn’t list Tape drive but only displays the direct attached drives if present or a blank table if none are connected.
11. Importing Foreign Configuration while Rebuild is in progress then query for Show fall the output would display multiple R60 VDs.
12. For any operation (Migrate/Init/BGI/CC) percentile completed in minutes is not displayed in StorCLI output. 
13. ‘All VD initialization’ command when run through StorCLI utility, shows the error message as failed for cachecaded VD.
14. While reconstruction is in progress, start of CC/Init/BGI operations on same VD throws an inappropriate error message.
15. In controller show cc the field CC current state will change only when it meets the schedule CC parameters.
16. All the unsupported commands for SWR controller if tried to execute may result in unknown behavior for example – system hang-up. For the list of unsupported commands refer to user guide Appendix C: Unsupported Commands in Embedded RAID.
17. Output for controller information contains junk characters in VMware ESXi 4.1 update2.  
18. FDE drives are displayed as secured drives on SWR- SCU controller.



Installation Commands: 
=======================
Refer to the User's Guide included in the package.



